Data Fields
gatts_noti_ind_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Server » Structures

GATT sending Notification or Indication event param description. More...

`#include <ble_gatts.h>`

## Data Fields
gatt_evt_type_t | type
uint16_t | handle
uint16_t | length
uint8_t * | value

## Detailed Description

GATT sending Notification or Indication event param description.

## Field Documentation

## ◆ handle

uint16_t gatts_noti_ind_t::handle

Characteristic Value handle to be notified or indicated.

## ◆ length

uint16_t gatts_noti_ind_t::length

Length of Characteristic Value to be sent.

## ◆ type

gatt_evt_type_t gatts_noti_ind_t::type

Request type (Notification/Indication). see gatt_evt_type_t.

## ◆ value

uint8_t* gatts_noti_ind_t::value

Characteristic Value pointer.

The documentation for this struct was generated from the following file:

- ble_gatts.h