Data Fields
gap_ext_init_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Extended initiating parameters. More...

`#include <ble_gapm.h>`

## Data Fields
uint8_t | type
uint8_t | prop
uint16_t | conn_to
gap_scan_wd_op_param_t | scan_param_1m
gap_scan_wd_op_param_t | scan_param_coded
gap_ext_conn_param_t | conn_param_1m
gap_ext_conn_param_t | conn_param_2m
gap_ext_conn_param_t | conn_param_coded
gap_bdaddr_t | peer_addr

## Detailed Description

Extended initiating parameters.

## Field Documentation

## ◆ conn_param_1m

gap_ext_conn_param_t gap_ext_init_param_t::conn_param_1m

Connection parameters for LE 1M PHY.

## ◆ conn_param_2m

gap_ext_conn_param_t gap_ext_init_param_t::conn_param_2m

Connection parameters for LE 2M PHY.

## ◆ conn_param_coded

gap_ext_conn_param_t gap_ext_init_param_t::conn_param_coded

Connection parameters for LE Coded PHY.

## ◆ conn_to

uint16_t gap_ext_init_param_t::conn_to

Timeout for automatic connection establishment (in unit of 10ms). Cancel the procedure if connection has not been connected when the timeout occurs. 0 means there is no timeout.

## ◆ peer_addr

gap_bdaddr_t gap_ext_init_param_t::peer_addr

Address of peer device in case white list is not used for connection.

## ◆ prop

uint8_t gap_ext_init_param_t::prop

Properties for the initiating procedure (see enum gap_init_prop_t for bit signification).

## ◆ scan_param_1m

gap_scan_wd_op_param_t gap_ext_init_param_t::scan_param_1m

Scan window opening parameters for LE 1M PHY.

## ◆ scan_param_coded

gap_scan_wd_op_param_t gap_ext_init_param_t::scan_param_coded

Scan window opening parameters for LE Coded PHY.

## ◆ type

uint8_t gap_ext_init_param_t::type

Initiating type (see enum gap_init_type_t).

The documentation for this struct was generated from the following file:

- ble_gapm.h