Data Fields
bas_c_handles_t Struct Reference
BLE Services » Battery Service Client (BAS_C) » Structures

Handles on the connected peer device needed to interact with it. More...

`#include <bas_c.h>`

## Data Fields
uint16_t | bas_srvc_start_handle
uint16_t | bas_srvc_end_handle
uint16_t | bas_bat_level_handle
uint16_t | bas_bat_level_cccd_handle
uint16_t | bas_bat_level_pres_handle

## Detailed Description

Handles on the connected peer device needed to interact with it.

## Field Documentation

## ◆ bas_bat_level_cccd_handle

uint16_t bas_c_handles_t::bas_bat_level_cccd_handle

BAS CCCD handle of Battery Level characteristic which has been got from peer.

## ◆ bas_bat_level_handle

uint16_t bas_c_handles_t::bas_bat_level_handle

BAS Battery Level characteristic Value handle which has been got from peer.

## ◆ bas_bat_level_pres_handle

uint16_t bas_c_handles_t::bas_bat_level_pres_handle

BAS Presentation Format Descriptor handle of Battery Level characteristic which has been got from peer.

## ◆ bas_srvc_end_handle

uint16_t bas_c_handles_t::bas_srvc_end_handle

BAS Service end handle.

## ◆ bas_srvc_start_handle

uint16_t bas_c_handles_t::bas_srvc_start_handle

BAS Service start handle.

The documentation for this struct was generated from the following file:

- bas_c.h