Enumerations
HAL I2S state
Peripheral Driver » HAL Driver » I2S » Enumerations

## Enumerations
enum | hal_i2s_state_t { HAL_I2S_STATE_RESET = 0x00, HAL_I2S_STATE_READY = 0x01, HAL_I2S_STATE_BUSY = 0x02, HAL_I2S_STATE_BUSY_TX = 0x12, HAL_I2S_STATE_BUSY_RX = 0x22, HAL_I2S_STATE_BUSY_TX_RX = 0x32, HAL_I2S_STATE_ABORT = 0x08, HAL_I2S_STATE_ERROR = 0x04 }
| HAL I2S State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_i2s_state_t

enum hal_i2s_state_t

HAL I2S State Enumerations definition.

Enumerator
HAL_I2S_STATE_RESET | Peripheral not initialized
HAL_I2S_STATE_READY | Peripheral initialized and ready for use
HAL_I2S_STATE_BUSY | An internal process is ongoing
HAL_I2S_STATE_BUSY_TX | Data Transmission process is ongoing
HAL_I2S_STATE_BUSY_RX | Data Reception process is ongoing
HAL_I2S_STATE_BUSY_TX_RX | Data Transmission and Reception process is ongoing
HAL_I2S_STATE_ABORT | Peripheral with abort request ongoing
HAL_I2S_STATE_ERROR | Peripheral in error