Modules | Macros
Defines
BLE Services » Health Thermometer Service (HTS)

## Modules
| Characteristics Mask
| Bit masks for the initialization of hts_init_t::char_mask.

## Macros
#define | HTS_CONNECTION_MAX
#define | HTS_TEM_MEAS_MAX_LEN 20
#define | HTS_TEM_TYPE_MAX_LEN 1
#define | HTS_INTM_TEM_MAX_LEN 20
#define | HTS_MEAS_INTERVAL_MAX_LEN 2
#define | HTS_MEAS_INTV_DFLT_MIN 2
#define | HTS_MEAS_INTV_DFLT_MAX 10

## Detailed Description

## Macro Definition Documentation

## ◆ HTS_CONNECTION_MAX

#define HTS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Health Thermometer Service connections.

## ◆ HTS_INTM_TEM_MAX_LEN

#define HTS_INTM_TEM_MAX_LEN 20

Maximun length of intermediate temperature encode.

## ◆ HTS_MEAS_INTERVAL_MAX_LEN

#define HTS_MEAS_INTERVAL_MAX_LEN 2

Maximum length of measurement interval value.

## ◆ HTS_MEAS_INTV_DFLT_MAX

#define HTS_MEAS_INTV_DFLT_MAX 10

Maximum interval of temperature measurement (in unit of 1s).

## ◆ HTS_MEAS_INTV_DFLT_MIN

#define HTS_MEAS_INTV_DFLT_MIN 2

Minimun interval of temperature measurement (in unit of 1s).

## ◆ HTS_TEM_MEAS_MAX_LEN

#define HTS_TEM_MEAS_MAX_LEN 20

Maximum length of temperature measurement encode.

## ◆ HTS_TEM_TYPE_MAX_LEN

#define HTS_TEM_TYPE_MAX_LEN 1

Maximum length of temperature type value.