Data Structures
Here are the data structures with brief descriptions:
[detail level 12]

C_adc_callback | HAL ADC Callback function definition
C_adc_handle | ADC handle Structure definition
C_aes_callback | HAL AES Callback function definition
C_aes_handle | AES handle Structure definition
C_aes_init | AES Init Structure definition
C_aon_gpio_callback | HAL AON_GPIO Callback function definition
C_aon_gpio_init | AON_GPIO init structure definition
C_aon_wdt_callback | HAL_AON_WDT Callback function definition
C_aon_wdt_handle | AON_WDT handle Structure definition
C_aon_wdt_init | AON_WDT_Configuration init structure definition
C_calendar_alarm | CALENDAR_Alarm calendar alarm structure definition
C_calendar_handle | CALENDAR handle Structure definition
C_calendar_time | CALENDAR_Time calendar time structure definition
C_cgc_init | CGC init structure definition
C_comp_callback | HAL COMP Callback function definition
C_comp_handle | COMP handle Structure definition
C_dma_handle | DMA handle Structure definition
C_dma_init | DMA Configuration Structure definition
C_dual_timer_handle | DUAL_TIMER handle Structure definition
C_dual_timer_init | DUAL TIMER init Structure definition
C_efuse_handle | EFuse handle Structure definition
C_efuse_init | EFuse init Structure definition
C_exflash_handle | ExFlash handle Structure definition
C_gpio_init | GPIO init structure definition
C_hal_calendar_callback | HAL_CALENDAR Callback function definition
C_hal_callback | HAL_HAL Callback function definition
C_hal_dual_timer_callback | HAL_DUAL_TIMER Callback function definition
C_hal_efuse_callback | HAL_EFUSE Callback function definition
C_hal_exflash_callback | HAL_EXFLASH Callback function definition
C_hal_gpio_callback | HAL_GPIO Callback function definition
C_hal_hmac_callback | HAL_HMAC Callback function definition
C_hal_i2c_callback | HAL_I2C Callback function definition
C_hal_i2s_callback | HAL_I2S Callback function definition
C_hal_pkc_callback | HAL_PKC Callback function definition
C_hal_pwm_callback | HAL_PWM Callback function definition
C_hal_pwr_handler | PWR callback handle Structure definition
C_hal_qspi_callback | HAL_QSPI Callback function definition
C_hal_rng_callback | HAL_RNG Callback function definition
C_hal_spi_callback | HAL_SPI Callback function definition
C_hal_timer_callback | HAL_TIMER Callback function definition
C_hal_uart_callback | HAL_UART Callback function definition
C_hal_wdt_callback | HAL_WDT Callback function definition
C_hal_xqspi_callback | HAL_XQSPI Callback function definition
C_hmac_handle | HMAC handle Structure definition
C_hmac_init | HMAC init Structure definition
C_i2c_handle | I2C handle Structure definition
C_i2c_init | I2C Configuration Structure definition
C_i2s_handle | I2S handle Structure definition
C_i2s_init | I2S init Structure definition
C_iso7816_callback | HAL_ISO7816 Callback function definition
C_iso7816_handle_t | ISO7816 handle Structure definition
C_keyram_mask | EFuse Keyram Structure definition
C_ll_adc_init | LL ADC init Structure definition
C_ll_aes_init | LL AES Init Structure definition
C_ll_aon_gpio_init | LL AON_GPIO init Structure definition
C_ll_cgc_init_t | LL CGC init Structure definition
C_ll_comp_init | LL COMP init Structure definition
C_ll_dma_init | LL DMA init Structure definition
C_ll_dual_timer_init | LL DUAL TIMER init Structure definition
C_ll_ecc_curve_init | LL PKC ECC P-256 Elliptic Curve Init Structure definition
C_ll_ecc_point | LL PKC ECC Point Structure definition
C_ll_gpio_init | LL GPIO init configuration definition
C_ll_hmac_init_t | LL HMAC Init Structure definition
C_ll_i2c_init | LL I2C init Structure definition
C_ll_i2s_init_t | LL I2S init structures definition
C_ll_iso7816_init | ISO7816_LL_init_structure LL ISO7816 init Structure definition
C_ll_msio_init | LL MSIO init Structure definition
C_ll_pkc_init | LL PKC Init Structure definition
C_ll_pwm_channel_init_t | LL PWM Output Channel init Structure definition
C_ll_pwm_init_t | LL PWM init Structure definition
C_ll_qspi_init_t | QSPI init structures definition
C_ll_rng_init | LL RNG Init Structure definition
C_ll_spim_init_t | LL SPIM init structures definition
C_ll_spis_init_t | SPIS init structures definition
C_ll_timer_init_t | LL TIMER init Structure definition
C_ll_uart_init_t | LL UART init Structure definition
C_ll_xqspi_init_t | XQSPI init structures definition
C_msio_init | MSIO init structure definition
C_pkc_big_number_add | PKC Big Number Addition expression input
C_pkc_big_number_multi | PKC Big Number Multiplication expression input
C_pkc_ecc_point_multi | PKC ECC Point Multiplication expression input
C_pkc_handle | PKC handle Structure definition
C_pkc_modular_add | PKC Modular Addition expression input
C_pkc_modular_compare | PKC Modular Comparison expression input
C_pkc_modular_shift | PKC Modular Left Shift expression input
C_pkc_modular_sub | PKC Modular Subtraction expression input
C_pkc_montgomery_inversion | PKC Montgomery Inversion expression input
C_pkc_montgomery_multi | PKC Montgomery Modular Multiplication expression input
C_pkc_rsa_modular_exponent | PKC RSA Modular Exponentiation expression input
C_qspi_command_t | QSPI command Structure definition
C_qspi_handle | QSPI handle Structure definition
C_qspi_init_t | QSPI init Structure definition
C_rng_handle | RNG handle Structure definition
C_rng_init | RNG init structure definition
C_spi_handle | SPI handle Structure definition
C_spi_init | SPI init Structure definition
C_timer_handle | TIMER handle Structure definition
C_timer_init | TIMER init Structure definition
C_uart_handle | UART handle Structure definition
C_uart_init | UART init structure definition
C_wdt_handle | WDT handle Structure definition
C_wdt_init | WDT init structure definition
C_xqspi_command_t | XQSPI command Structure definition
C_xqspi_handle_t | XQSPI handle Structure definition
C_xqspi_init_t | XQSPI init Structure definition
C adc_trim_info_t | ADC trim parameter information definition
C ags_ack_packet_t | Alexa Gadget Service ACK packet
C ags_evt_t | Alexa Gadget Service event
C ags_header_base_t | Alexa Gadget Service base part of data packet header
C ags_header_first_ext_t | Alexa Gadget Service extended version of header in first packet
C ags_header_first_t | Alexa Gadget Service header in first packet
C ags_header_subs_ext_t | Alexa Gadget Service extended version of header in subsequent packets
C ags_header_subs_t | Alexa Gadget Service header in subsequent packets
C ags_init_t | Alexa Gadget Service init stucture. This contains all option and data needed for initialization of the service
C ags_stream_env_t | Alexa Gadget Service gadget stream enviorenment variable
C ams_c_attr_info_t | Structure that stores attribute information
C ams_c_cmd_list_t | Structure that stores new command list
C ams_c_cplt_attr_data_t | Complete attribution's value
C ams_c_ett_attr_id_t | Structure that stores the attribute to be concerned or to display completely
C ams_c_evt_t | Apple Media Service Client event
C ams_c_handles_t | Handles on the connected peer device needed to interact with it
C ancs_c_att_handles_t | Ancs handle structure
C ancs_c_evt_t | ANCS Client event
C ancs_ntf_flags_t | Notification flags that can be performed for iOS notifications
C ans_c_ctrl_pt_t | Alert Notification Service Client Control Point value
C ans_c_evt_t | Alert Notification Service Client event
C ans_c_handles_t | Handles on the connected peer device needed to interact with it
C ans_c_new_alert_t | Alert Notification Service Client decoded New Alert value
C ans_c_unread_alert_t | Alert Notification Service Client decoded Unread Alert Status value
C ans_ctrl_pt_t | Alert Notification Service Control Point value
C ans_evt_t | Alert Notification Service event
C ans_init_t | Alert Notification Service init stucture. This contains all options and data needed for initialization of the service
C ans_new_alert_t | Alert Notification Service New Alert value
C ans_unread_alert_t | Alert Notification Service Unread Alert Status value
C app_adc_evt_t | ADC event structure definition
C app_adc_mode_t | ADC operate mode Structures
C app_adc_params_t | ADC parameters structure definition
C app_adc_pin_cfg_t | ADC pins config Structures
C app_adc_pin_t | ADC pins Structures
C app_aes_evt_t | AES event structure definition
C app_aes_params_t | AES parameters structure definition
C app_callback_t | The app callbacks for GAP, GATT, SM and L2CAP
C app_comp_params_t | COMP parameters structure definition
C app_comp_pin_cfg_t | COMP pins config Structures
C app_comp_pin_t | COMP pins Structures
C app_dma_params_t | DMA parameters structure definition
C app_dual_tim_params_t | DUAL_TIM parameters structure definition
C app_gpiote_evt_t | GPIO Interrupt event Structure definition
C app_gpiote_param_t | GPIOTE Interrupt parameters structure definition
C app_hmac_evt_t | HMAC event structure definition
C app_hmac_params_t | HMAC parameters structure definition
C app_i2c_evt_t | I2C event structure definition
C app_i2c_mode_t | I2C operate mode Enumerations definition
C app_i2c_params_t | I2C parameters structure definition
C app_i2c_pin_cfg_t | I2C IO configuration Structures
C app_i2c_pin_t | I2C IO Structures
C app_i2s_evt_t | I2S event structure definition
C app_i2s_mode_t | I2S operate mode Enumerations definition
C app_i2s_params_t | I2S parameters structure definition
C app_i2s_pin_cfg_t | I2S IO configuration Structures
C app_i2s_pin_t | I2S IO Structures
C app_io_init_t | GPIO parameter structure definition
C app_pkc_evt_t | PKC event structure definition
C app_pkc_params_t | PKC parameters structure definition
C app_pwm_channel_init_t | PWM Channel init Structure definition
C app_pwm_params_t | PWM parameters structure definition
C app_pwm_pin_cfg_t | PWM configuration Structures
C app_pwm_pin_t | PWM IO configuration Structures
C app_qspi_evt_t | QSPI event structure definition
C app_qspi_mode_t | QSPI operate mode Enumerations definition
C app_qspi_params_t | QSPI parameters structure definition
C app_qspi_pin_cfg_t | QSPI configuration Structures
C app_qspi_pin_t | QSPI IO configuration Structures
C app_rng_evt_t | RNG event structure definition
C app_rng_params_t | RNG parameters structure definition
C app_rtc_evt_t | RTC event structure definition
C app_sleep_callbacks_t | PWR sleep check function Structure
C app_spi_evt_t | SPI event structure definition
C app_spi_mode_t | SPI operate mode Enumerations definition
C app_spi_params_t | SPI parameters structure definition
C app_spi_pin_cfg_t | SPI IO configuration Structures
C app_spi_pin_t | SPI IO Structures
C app_tim_params_t | TIM parameters structure definition
C app_uart_evt_t | UART event structure definition
C app_uart_mode_t | UART operate mode Enumerations definition
C app_uart_params_t | UART parameters structure definition
C app_uart_pin_cfg_t | UART IO configuration Structures
C app_uart_pin_t | UART IO Structures
C app_uart_tx_buf_t | UART buffer structure definition
C attm_desc_128_t | Service(128 bits UUID) description
C attm_desc_t | Service(16-bit UUID) description
C bas_c_evt_t | Battery Service Client event
C bas_c_handles_t | Handles on the connected peer device needed to interact with it
C bas_evt_t | Battery Service event
C bas_init_t | Battery Service init structure. This contains all options and data needed for initialization of the service
C bcs_evt_t | Body Composition Service event
C bcs_init_t | Body Composition Service Init variable
C bcs_meas_flag_t | Body composition Measurement flag data
C bcs_meas_val_t | Body composition Measurement data
C birth_date_t | UDS Characteristic - birthdate's structure
C ble_dis_c_read_rsp_t | Device Information Service Client Read Response encode structure
C ble_escs_init_params_t | EddyStone Configuration Service environment variable
C ble_gattc_browse_srvc_t | GATTC Browse service(s) indication
C ble_gattc_char_desc_disc_t | GATT characteristic descriptor discovery
C ble_gattc_char_disc_t | GATT characteristic discovery
C ble_gattc_char_t | GATT characteristic
C ble_gattc_desc_t | GATT descriptor
C ble_gattc_incl_disc_t | GATT include discovery
C ble_gattc_include_t | GATT include
C ble_gattc_ntf_ind_t | GATTC Notification and Indication value indication
C ble_gattc_read_rsp_t | GATT value Read response
C ble_gattc_read_value_t | GATT Client Read value
C ble_gattc_service_t | GATT service
C ble_gattc_srvc_disc_t | GATT service discovery
C ble_gattc_write_t | GATT Client Write
C ble_gatts_ntf_ind_t | GATTS Operation Complete event structure
C ble_prf_manager_cbs_t | Profile manager callbacks
C ble_sch_config_t | BLE Scheduler configure defination
C ble_slp_config_t | BLE Sleep configure defination
C ble_uuid_t | GATT UUID structure
C bond_dev_list_t | Bonded device list
C boot_info_t | BootLoader information definition
C bps_init_t | Blood Pressure Service init stucture. This contains all option and data needed for initialization of the service
C bps_meas_t | Blood Pressure measurement structure
C cscs_evt_t | Cycling Speed and Cadence Service event
C cscs_init_t | Cycling Speed and Cadence Service init stucture. This contains all option and data needed for initialization of the service
C cscs_meas_val_t | Cycling Speed and Cadence Measurement Character value structure
C cts_adj_info_t | CTS Adjust information
C cts_c_cur_time_t | Current Time value
C cts_c_evt_t | Current Time Service Client event
C cts_c_exact_time_256_t | Exact Time 256
C cts_c_handles_t | Handles on the connected peer device needed to interact with it
C cts_c_loc_time_info_t | Local Time Information
C cts_c_ref_time_info_t | Reference Time Information
C cts_cur_time_t | CTS Current Time value
C cts_evt_t | Current Time Service event
C cts_exact_time_256_t | CTS Exact Time 256
C cts_init_t | Current Time Service init structure. This contains all option and data needed for initialization of the service
C cts_loc_time_info_t | CTS Local Time Information
C cts_ref_time_info_t | CTS Reference Time Information
C dfu_adv_name_info_t | DFU Advertisement name config definition
C dfu_cmd_disable_t | DFU cmd disable info definition
C dfu_func_t | DFU used functions config definition
C dfu_nvds_info_t | DFU NVDS init info definition
C dfu_pro_callback_t | DFU program state callback definition
C dfu_spi_flash_func_t | SPI used functions config definition
C dfu_uart_info_t | DFU uart config definition
C dis_c_evt_t | Device Information Service Client event
C dis_c_handles_t | Handles on the connected peer device needed to interact with it
C dis_c_pnp_id_t | Response data for PnP ID parameters
C dis_c_reg_cert_data_list_t | Response data for IEEE 11073-20601 Regulatory Certification Data List Structure
C dis_c_string_t | Response data for string-based DIS characteristics
C dis_c_sys_id_t | Response data for System ID parameters
C dis_init_t | Device Information Service init structure. This contains all options and data needed for initialization of the service
C dis_pnp_id_t | PnP ID parameters
C dis_reg_cert_data_list_t | IEEE 11073-20601 Regulatory Certification Data List Structure
C dis_string_t | UTF-8 string data type
C dis_sys_id_t | System ID parameters. The first field is the LSOs and the second field contains the MSOs
C dss_evt_t | Device Synchronize Service Synchronize event
C escs_eid_t | Structure for storing EID slot key
C fast_otas_evt_t | FAST_OTA Service event
C fast_otas_init_t | FAST_OTA Service initialization variable
C FPB_REG_TypeDef | FPB register
C gap_addr_t | The struct of address
C gap_adv_param_t | Advertising parameters for legacy advertising
C gap_adv_period_cfg_t | Configuration for periodic advertising
C gap_adv_prim_cfg_t | Configuration for advertising on primary channel
C gap_adv_second_cfg_t | Configuration for advertising on secondary channel
C gap_adv_time_param_t | Advertising timing parameter
C gap_bdaddr_t | The struct of broadcast address with broadcast type
C gap_cb_fun_t | The gap callback function struct
C gap_chnl_map_t | Channel map structure
C gap_con_plan_tag_t | The Structure for BLE Connection Arrangement
C gap_conn_cmp_t | Connection complete info
C gap_conn_info_param_t | The info of connecting operation
C gap_conn_info_t | Connection info
C gap_conn_param_t | The parameter of connection
C gap_conn_update_cmp_t | Connection parameter used to update connection parameters
C gap_conn_update_param_t | The parameter of update connection
C gap_dev_adv_tx_power_t | TX power info struct
C gap_dev_info_get_t | Get device info operation struct
C gap_dev_info_t | Device info
C gap_dev_rf_path_comp_ind_t | RF path compensation values info
C gap_dev_tx_power_t | TX power info struct
C gap_dev_version_ind_t | The struct of device version
C gap_ext_adv_param_t | Advertising parameters for extended advertising and periodic advertising
C gap_ext_adv_report_ind_t | APP receives the extended advertising report indication info struct
C gap_ext_conn_param_t | Connection parameters
C gap_ext_init_param_t | Extended initiating parameters
C gap_ext_scan_param_t | Parameters for extended scanning
C gap_get_bd_addr_t | Get broadcast address struct
C gap_init_param_t | Legacy initiating parameters
C gap_le_phy_ind_t | PHY info
C gap_le_pkt_size_ind_t | Supported data length size Indication
C gap_lepsm_register_t | LE Protocol/Service Multiplexer information
C gap_max_adv_data_len_ind_t | Maximum advertising data length info
C gap_max_data_len_t | Max data length info struct
C gap_nb_adv_sets_t | Number of available advertising sets info
C gap_peer_features_ind_t | LE features info
C gap_peer_info_param_t | Get peer info operation struct
C gap_peer_info_t | LE peer info
C gap_peer_name_ind_t | Name of peer device indication
C gap_peer_version_ind_t | Peer version info
C gap_per_sync_param_t | Periodic advertising synchronization parameters
C gap_period_adv_addr_cfg_t | Periodic advertising information
C gap_ral_dev_info_t | RPA list item info
C gap_rslv_addr_read_t | Read resolvable address info struct
C gap_scan_param_t | Parameters for legacy scanning
C gap_scan_wd_op_param_t | Scan Window operation parameters
C gap_sec_key_t | Security key
C gap_set_pref_slave_evt_dur_param_t | Set preference slave event duration
C gap_slv_pref_t | Slave preferred connection parameters
C gap_sugg_dflt_data_len_t | Suggested default data length info
C gap_sync_established_ind_t | Sync established indication
C gatt_common_cb_fun_t | GATT common callback function description
C gattc_browse_attr_char_t | GATTC Browse information about Characteristic
C gattc_browse_attr_info | GATTC Browse attribute information
C gattc_browse_attr_t | GATTC Browse information about Attribute
C gattc_browse_inc_srvc_t | GATTC Browse information about Included Service
C gattc_cb_fun_t | GATTC Event callback Structures
C gattc_disc_char_t | GATTC discovery characteristic structure
C gattc_prf_cbs_t | GATTC Profile callback Structures
C gattc_prf_reg_peer_evt_t | GATTC profile register to peer event info structure
C gattc_read_by_uuid_t | GATTC read by characteristic UUID structure
C gattc_read_multiple_t | GATTC Read Multiple
C gattc_write_attr_value_t | GATTC write attribute value structure
C gattc_write_no_resp_t | GATTC write without response structure
►C gatts_create_db_t | Parameter of Added service description
C attribute_table |
C gatts_noti_ind_t | GATT sending Notification or Indication event param description
C gatts_prep_write_cfm_t | GATT prepare write result description
C gatts_prep_write_req_cb_t | GATT prepare write request struct
C gatts_prf_cbs_t | GATT server callback function in relation to a profile
C gatts_read_cfm_t | GATT read attribute result description
C gatts_read_req_cb_t | GATT read request struct
C gatts_write_cfm_t | GATT write attribute result description
C gatts_write_req_cb_t | GATT write request struct
C gdx_lcp_config_t | LCP Parameter
C gls_evt_t | Glucose Service event
C gls_init_t | Glucose Service init stucture. This contains all option and data needed for initialization of the service
C gls_meas_ctx_t | Glucose measurement context structure
C gls_meas_val_t | Glucose Measurement structure. This contains glucose measurement value
C gls_racp_filter_t | Glucose Recoerd Access Control Point filter value
C gls_racp_req_t | Glucose Recoerd Access Control Point request value
C gls_racp_rsp_t | Glucose Recoerd Access Control Point response value
C gls_rec_t | Glucose measurement record
C gr55xx_chip_config_t | GR55XX Chip configure defination
C gus_c_evt_t | Goodix UART Service Client event
C gus_c_handles_t | Handles on the connected peer device needed to interact with it
C gus_evt_t | Goodix UART Service event
C gus_init_t | Goodix UART Service init stucture. This contains all option and data needed for initialization of the service
C hci_uart_call_t | The function pointers for HCI UART
C hids_evt_t | HID Service event
C hids_hid_info_t | HID Information characteristic value
C hids_init_t | HID Service initialization variable
C hids_report_int_t | HID Service Report characteristic define
C hids_report_map_t | HID Service Report Map characteristic value
C hids_report_ref_t | Value of a Report Reference descriptor
C hrrcps_evt_t | HRS RSCS Relay Control Point Service event
C hrrcps_rsp_val_t | HRS RSCS Relay Control Point Response value
C hrs_c_evt_t | Heart Rate Service Client event
C hrs_c_handles_t | Handles on the connected peer device needed to interact with it
C hrs_c_hr_meas_t | Heart Rate Measurement characteristic value structure
C hrs_evt_t | Heart Rate Service event
C hrs_init_t | Heart Rate Service Init variable
C hts_evt_t | Health Thermometer Service event
C hts_init_t | Health Thermometer Service init stucture. This contains all option and data needed for initialization of the service
C hts_meas_val_t | Health Theromometer Measurement Character value structure
C ias_c_evt_t | Immediate Alert Service Client event
C ias_c_handles_t | Handles on the connected peer device needed to interact with it
C ias_evt_t | Immediate Alert Service event
C ias_init_t | Immediate Alert Service init stucture. This contains all option and data needed for initialization of the service
C ieee_float16_t | SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent
C ieee_float32_t | SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent
C iso7816_init_t | ISO7816_init_structure ISO7816 init structure definition
C l2cap_lecb_cb_fun_t | Callback registered by APP
C lecb_add_credits_ind_t | LE credit based connection addition indication
C lecb_add_credits_t | LE flow control credit packet parameter.
C lecb_cfm_conn_t | LE credit based connection confirm parameter
C lecb_conn_ind_t | LE credit based connection created indication
C lecb_conn_req_ind_t | Receive LE credit based connection request packet indication
C lecb_conn_req_t | The parameter of LE credit based connection request packet sending
C lecb_disconn_ind_t | LE credit based disconnect indication
C lecb_sdu_send_evt_t | LE credit based SDU sending complete event
C lecb_sdu_t | SDU packet parameter
C link_rx_info_t | Link RX information definition
C lls_c_evt_t | Link Loss Service Client event
C lls_c_handles_t | Handles on the connected peer device needed to interact with it
C lls_evt_t | Link Loss Service event
C lls_init_t | Link Loss Service init stucture. This contains all option and data needed for initialization of the service
C lns_evt_t | Log Notification Service event
C lns_log_data_t | Log Information data
C ndcs_time_dst_t | Time with DST
C ntf_source_pdu_t | IOS notification structure
C otas_c_evt_t | OTA Service Client event
C otas_c_handles_t | Handles on the connected peer device needed to interact with it
C otas_evt_t | OTA Service event
C otas_init_t | OTA Service initialization variable
C pass_c_evt_t | Phone Alert Status Client Service event
C pass_c_handles_t | Handles on the connected peer device needed to interact with it
C pass_evt_t | Phone Alert Status Service event
C pass_init_t | Phone Alert Status Service init stucture. This contains all option and data needed for initialization of the service
C pcs_evt_t | PCS Service event
C pcs_init_t | PCS Service init stucture. This contains all option and data needed for initialization of the service
C period_adv_list_t | Periodic advertising list
C pkc_init_t | PKC Init Structure definition
C pmu_trim_info_t | PMU trim parameter information definition
C prf_att_info_t | Attribute information
C prf_char_pres_fmt_t | Characteristic Presentation Format Descriptor structure. The packed size is PRF_CHAR_PRES_FMT_SIZE
C prf_client_info_t | Profile client register information structure
C prf_date_time_t | The date and time structure. The packed size is 7 bytes
C prf_server_info_t | Profile server register information structure
C pwm_channel_init_t | PWM Channel init Structure definition
C pwm_handle_t | PWM handle Structure definition
C pwm_init_t | PWM init Structure definition
C pwr_mgmt_var_box_t | Power manager setting parameter. Use pwr_mgmt_var_set to transfer the parameters in the structure to PMU, and then the pwr_mgmt_mode_set function will use the new parameters for power management. Note that this is an advanced API, the wrong setting of parameters may lead to abnormal power management, so please use it carefully
C pwr_table_t | Parameter configuration table
C ral_dev_list_t | RPA list info
C read_multiple_t | Read Multiple Handles
C rf_trim_info_t | RF trim parameter information definition
C rscs_c_evt_t | Running Speed and Cadence Service Client event
C rscs_c_handles_t | Handles on the connected peer device needed to interact with it
C rscs_c_meas_val_t | Running Speed and Cadence Measurement Character value structure
C rscs_evt_t | Running Speed and Cadence Service event
C rscs_init_t | Running Speed and Cadence Service init stucture. This contains all option and data needed for initialization of the service
C rscs_meas_val_t | Running Speed and Cadence Measurement Character value structure
C rtus_evt_t | RTUS Event data
C rtus_init_t | Reference Time Update Service init structure. This contains all option and data needed for initialization of the service
C rtus_update_state_t | RTUS Time Update State
C samples_evt_t | Sample Service event
C samples_init_t | Sample Service init stucture. This contains all option and data needed for initialization of the service
C sdk_version_t | SDK version definition
C sec_cb_fun_t | SEC register call back
C sec_cfm_enc_data_t | SEC Confirm encryption data
C sec_cfm_enc_t | SEC Confirm encryption
C sec_enc_req_data_t | SEC encryption request data
C sec_enc_req_t | SEC encryption request
C sec_nc_t | SEC number comparison value
C sec_oob_t | SEC OOB value
C sec_param_t | SEC Parameter
C sec_tk_t | TK value
C slot_lock_code_t | Structure for storing a slot key
C stack_heaps_table_t | The table contains the pointers to four arrays which are used as heap memory by BLE stack in ROM. The size of four arrays depends on the number of connections and the number of attributes of profiles
C sys_assert_cb_t | Assert callbacks
C ths_c_evt_t | Throughput Service Client event
C ths_c_handles_t | Handles on the connected peer device needed to interact with it
C ths_evt_t | Throughput Service event
C ths_init_t | Throughput Service init stucture. This contains all option and data needed for initialization of the service
C thscps_adv_param_t | THS Control Point Advertising Parameters
C thscps_evt_t | THS Control Point Service event
C thscps_rsp_val_t | THS Control Point Response value
C thscps_setting_t | THS Setting Information value
C thscps_test_conn_info_t | THS connect Information value
C thscps_test_info_t | THS Test Information value
C tps_c_evt_t | Tx Power Service Client event
C tps_c_handles_t | Handles on the connected peer device needed to interact with it
C tps_init_t | Tx Power Servic init stucture. This contains all option and data needed for initialization of the service
C uds_chars_flag_t | UDS Characteristics Flags structure
C uds_chars_val_t | UDS Characteristics value structure
C uds_evt_t | User Data Service event
C uds_init_t | User Data Service init structure. This contains all option and data needed for initialization of the service
C uds_regi_user_data_flag_t | Registered User Data Flags structure
C uds_regi_user_data_stream_t | UDS Registered User Data stream
C wechat_data_t | WeChat service data
C wechat_evt_t | WeChat Service event
C wechat_init_t | WeChat Service Init variable
C wechat_pedo_meas_t | WeChat current pedometer measurement variable
C wechat_pedo_target_t | WeChat pedometer target variable
C white_list_t | White list
C wss_evt_t | Weight Scale Service event
C wss_init_t | Weight Scale Service Init variable
C wss_meas_val_t | Weight Scale Measurement data