Macros
QSPI Buad Rate
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_BAUD_RATE_64M 0x00000000UL
#define | LL_XQSPI_BAUD_RATE_48M (1UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
#define | LL_XQSPI_BAUD_RATE_32M (2UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
#define | LL_XQSPI_BAUD_RATE_24M (3UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)
#define | LL_XQSPI_BAUD_RATE_16M (4UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_BAUD_RATE_16M

#define LL_XQSPI_BAUD_RATE_16M (4UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 16MHz

## ◆ LL_XQSPI_BAUD_RATE_24M

#define LL_XQSPI_BAUD_RATE_24M (3UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 24MHz

## ◆ LL_XQSPI_BAUD_RATE_32M

#define LL_XQSPI_BAUD_RATE_32M (2UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 32MHz

## ◆ LL_XQSPI_BAUD_RATE_48M

#define LL_XQSPI_BAUD_RATE_48M (1UL << AON_PWR_REG01_XF_SCK_CLK_SEL_Pos)

Clock to 48MHz

## ◆ LL_XQSPI_BAUD_RATE_64M

#define LL_XQSPI_BAUD_RATE_64M 0x00000000UL

Clock to 64MHz