Macros
Action state
Peripheral Driver » HAL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | HAL_ISO7816_ACTION_NONE LL_ISO7816_ACTION_NONE
#define | HAL_ISO7816_ACTION_OFF LL_ISO7816_ACTION_OFF
#define | HAL_ISO7816_ACTION_STOPCLK LL_ISO7816_ACTION_STOPCLK
#define | HAL_ISO7816_ACTION_ON LL_ISO7816_ACTION_ON
#define | HAL_ISO7816_ACTION_WARMRST LL_ISO7816_ACTION_WARMRST
#define | HAL_ISO7816_ACTION_RX LL_ISO7816_ACTION_RX
#define | HAL_ISO7816_ACTION_TX LL_ISO7816_ACTION_TX
#define | HAL_ISO7816_ACTION_TXRX LL_ISO7816_ACTION_TXRX

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_ISO7816_ACTION_NONE

#define HAL_ISO7816_ACTION_NONE LL_ISO7816_ACTION_NONE

Do Nothing.

## ◆ HAL_ISO7816_ACTION_OFF

#define HAL_ISO7816_ACTION_OFF LL_ISO7816_ACTION_OFF

Switch Off.

## ◆ HAL_ISO7816_ACTION_ON

#define HAL_ISO7816_ACTION_ON LL_ISO7816_ACTION_ON

Switch on and receive ATR.

## ◆ HAL_ISO7816_ACTION_RX

#define HAL_ISO7816_ACTION_RX LL_ISO7816_ACTION_RX

Receive.

## ◆ HAL_ISO7816_ACTION_STOPCLK

#define HAL_ISO7816_ACTION_STOPCLK LL_ISO7816_ACTION_STOPCLK

Stop the clock.

## ◆ HAL_ISO7816_ACTION_TX

#define HAL_ISO7816_ACTION_TX LL_ISO7816_ACTION_TX

Transmit.

## ◆ HAL_ISO7816_ACTION_TXRX

#define HAL_ISO7816_ACTION_TXRX LL_ISO7816_ACTION_TXRX

Transmit, followed by RX.

## ◆ HAL_ISO7816_ACTION_WARMRST

#define HAL_ISO7816_ACTION_WARMRST LL_ISO7816_ACTION_WARMRST

Trigger warm reset and receive ATR.