Data Fields
lls_c_handles_t Struct Reference
BLE Services » Link Loss Service Client (LLS_C) » Structures

Handles on the connected peer device needed to interact with it. More...

`#include <lls_c.h>`

## Data Fields
uint16_t | lls_srvc_start_handle
uint16_t | lls_srvc_end_handle
uint16_t | lls_alert_level_handle

## Detailed Description

Handles on the connected peer device needed to interact with it.

## Field Documentation

## ◆ lls_alert_level_handle

uint16_t lls_c_handles_t::lls_alert_level_handle

LLS Alert Level characteristic Value handle which has been got from peer.

## ◆ lls_srvc_end_handle

uint16_t lls_c_handles_t::lls_srvc_end_handle

LLS Service end handle.

## ◆ lls_srvc_start_handle

uint16_t lls_c_handles_t::lls_srvc_start_handle

LLS Service start handle.

The documentation for this struct was generated from the following file:

- lls_c.h