Data Fields
gls_meas_val_t Struct Reference
BLE Services » Glucose Service (GLS) » Structures

Glucose Measurement structure. This contains glucose measurement value. More...

`#include <gls.h>`

## Data Fields
uint8_t | flags
uint16_t | sequence_number
prf_date_time_t | base_time
int16_t | time_offset
ieee_float16_t | glucose_concentration
uint8_t | type
uint8_t | sample_location
uint16_t | sensor_status_annunciation

## Detailed Description

Glucose Measurement structure. This contains glucose measurement value.

## Field Documentation

## ◆ base_time

prf_date_time_t gls_meas_val_t::base_time

Time stamp.

## ◆ flags

uint8_t gls_meas_val_t::flags

Flags.

## ◆ glucose_concentration

ieee_float16_t gls_meas_val_t::glucose_concentration

Glucose concentration.

## ◆ sample_location

uint8_t gls_meas_val_t::sample_location

Sample location.

## ◆ sensor_status_annunciation

uint16_t gls_meas_val_t::sensor_status_annunciation

Sensor status annunciation.

## ◆ sequence_number

uint16_t gls_meas_val_t::sequence_number

Sequence number.

## ◆ time_offset

int16_t gls_meas_val_t::time_offset

Time offset.

## ◆ type

uint8_t gls_meas_val_t::type

Type.

The documentation for this struct was generated from the following file:

- gls.h