Macros
GPIOEx Mux Mode definition
Peripheral Driver » HAL Driver » GPIOEx » Defines » GPIOEx Exported Constants

## Macros
#define | GPIO_MUX_0 LL_GPIO_MUX_0
#define | GPIO_MUX_1 LL_GPIO_MUX_1
#define | GPIO_MUX_2 LL_GPIO_MUX_2
#define | GPIO_MUX_3 LL_GPIO_MUX_3
#define | GPIO_MUX_4 LL_GPIO_MUX_4
#define | GPIO_MUX_5 LL_GPIO_MUX_5
#define | GPIO_MUX_6 LL_GPIO_MUX_6
#define | GPIO_MUX_7 LL_GPIO_MUX_7
#define | GPIO_MUX_8 LL_GPIO_MUX_8

## Detailed Description

## Macro Definition Documentation

## ◆ GPIO_MUX_0

#define GPIO_MUX_0 LL_GPIO_MUX_0

GPIO Mux mode 0

## ◆ GPIO_MUX_1

#define GPIO_MUX_1 LL_GPIO_MUX_1

GPIO Mux mode 1

## ◆ GPIO_MUX_2

#define GPIO_MUX_2 LL_GPIO_MUX_2

GPIO Mux mode 2

## ◆ GPIO_MUX_3

#define GPIO_MUX_3 LL_GPIO_MUX_3

GPIO Mux mode 3

## ◆ GPIO_MUX_4

#define GPIO_MUX_4 LL_GPIO_MUX_4

GPIO Mux mode 4

## ◆ GPIO_MUX_5

#define GPIO_MUX_5 LL_GPIO_MUX_5

GPIO Mux mode 5

## ◆ GPIO_MUX_6

#define GPIO_MUX_6 LL_GPIO_MUX_6

GPIO Mux mode 6

## ◆ GPIO_MUX_7

#define GPIO_MUX_7 LL_GPIO_MUX_7

GPIO Mux mode 7

## ◆ GPIO_MUX_8

#define GPIO_MUX_8 LL_GPIO_MUX_8

GPIO Mux mode 8