Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - p -

- P : _ll_ecc_curve_init
- p_A : _pkc_big_number_add , _pkc_big_number_multi , _pkc_modular_add , _pkc_modular_compare , _pkc_modular_shift , _pkc_modular_sub , _pkc_montgomery_inversion , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- p_B : _pkc_big_number_add , _pkc_big_number_multi , _pkc_modular_add , _pkc_modular_sub , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- p_buffer : _adc_handle , _i2c_handle
- p_cmd : ams_c_cmd_list_t
- p_cryp_input_buffer : _aes_handle
- p_cryp_output_buffer : _aes_handle
- p_data : ags_evt_t , ams_c_attr_info_t , ams_c_cplt_attr_data_t , bcs_evt_t , cscs_evt_t , cts_evt_t , dis_c_string_t , fast_otas_evt_t , gls_evt_t , gus_c_evt_t , gus_evt_t , hts_evt_t , lns_log_data_t , otas_c_evt_t , otas_evt_t , pcs_evt_t , prf_att_info_t , rscs_evt_t , samples_evt_t , ths_c_evt_t , ths_evt_t , thscps_setting_t , uds_evt_t , uds_regi_user_data_stream_t , wechat_data_t , wss_evt_t
- p_dev_mac : wechat_init_t
- p_digest : _hmac_handle
- p_dma : _adc_handle , _qspi_handle
- p_dmarx : _i2c_handle , _i2s_handle , _spi_handle , _uart_handle
- p_dmatx : _i2c_handle , _i2s_handle , _spi_handle , _uart_handle
- p_ecc_curve : _ll_pkc_init , pkc_init_t
- p_ecc_point : _pkc_ecc_point_multi
- p_first_name : uds_chars_val_t
- p_hash : _ll_hmac_init_t
- p_init_vector : _aes_init , _ll_aes_init
- p_instance : _aes_handle , _dual_timer_handle , _efuse_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pkc_handle , _qspi_handle , _rng_handle , _spi_handle , _timer_handle , _uart_handle , _wdt_handle , _xqspi_handle_t , pwm_handle_t
- p_K : _pkc_ecc_point_multi
- p_key : _aes_init , _hmac_init , _ll_aes_init , _ll_hmac_init_t
- p_kout : app_pkc_params_t
- p_list : dis_c_reg_cert_data_list_t , dis_reg_cert_data_list_t
- p_map : hids_report_map_t
- p_message : _hmac_handle
- p_P : _pkc_handle , _pkc_modular_add , _pkc_modular_compare , _pkc_modular_shift , _pkc_modular_sub , _pkc_montgomery_inversion , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- p_P_R2 : _pkc_rsa_modular_exponent
- p_parent : _dma_handle
- p_pnp_id : dis_init_t
- p_read_multiple : gattc_read_multiple_t
- p_result : _pkc_handle , app_pkc_params_t
- p_rx_buffer : _i2s_handle , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- p_seed : _aes_init , _ll_aes_init
- p_segm_length : uds_regi_user_data_stream_t
- p_str : dis_string_t
- p_sys_id : dis_init_t
- p_tx_buffer : _i2s_handle , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- p_tx_rx_buffer : _iso7816_handle_t
- p_user_hash : _hmac_init
- p_uuid : ble_gattc_char_t , ble_gattc_desc_t , ble_gattc_include_t , ble_gattc_service_t , gattc_disc_char_t , gattc_read_by_uuid_t
- p_value : ble_gattc_ntf_ind_t , ble_gattc_read_value_t , gattc_write_attr_value_t , gattc_write_no_resp_t
- p_xqspi : _exflash_handle
- packets_val : thscps_test_info_t
- page_size : dfu_nvds_info_t
- param : ams_c_evt_t , thscps_evt_t , wechat_evt_t
- parity : _ll_uart_init_t , _uart_init , dfu_uart_info_t
- pass_alert_status_cccd_handle : pass_c_handles_t
- pass_alert_status_handle : pass_c_handles_t
- pass_ringer_ctrl_pt_handle : pass_c_handles_t
- pass_ringer_set_cccd_handle : pass_c_handles_t
- pass_ringer_set_handle : pass_c_handles_t
- pass_srvc_end_handle : pass_c_handles_t
- pass_srvc_start_handle : pass_c_handles_t
- payload_length : ags_ack_packet_t , ags_header_first_ext_t , ags_header_first_t , ags_header_subs_ext_t , ags_header_subs_t
- pdu : thscps_test_conn_info_t
- pedo_target : wechat_evt_t
- peer_added_credits : lecb_add_credits_ind_t
- peer_addr : gap_adv_param_t , gap_conn_cmp_t , gap_ext_adv_param_t , gap_ext_init_param_t , gap_init_param_t , gap_peer_name_ind_t
- peer_addr_type : gap_conn_cmp_t
- peer_cid : lecb_cfm_conn_t , lecb_conn_req_ind_t
- peer_credits : lecb_conn_ind_t
- peer_features : gap_peer_info_t
- peer_info : gap_peer_info_param_t
- peer_irk : gap_ral_dev_info_t
- peer_mps : lecb_conn_ind_t , lecb_conn_req_ind_t
- peer_mtu : lecb_conn_ind_t , lecb_conn_req_ind_t
- peer_version : gap_peer_info_t
- per_sync_idx : gap_ext_adv_report_ind_t
- period : gap_ext_scan_param_t
- period_adv_intv : gap_ext_adv_report_ind_t
- period_cfg : gap_ext_adv_param_t
- perm : attm_desc_128_t , attm_desc_t
- phy : gap_adv_prim_cfg_t , gap_adv_second_cfg_t , gap_conn_info_t , gap_sync_established_ind_t , thscps_adv_param_t
- phy_prim : gap_ext_adv_report_ind_t
- phy_second : gap_ext_adv_report_ind_t
- pin : _aon_gpio_init , _gpio_init , _ll_aon_gpio_init , _ll_gpio_init , _ll_msio_init , _msio_init , app_adc_pin_t , app_comp_pin_t , app_gpiote_evt_t , app_gpiote_param_t , app_i2c_pin_t , app_i2s_pin_t , app_io_init_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t
- pin_cfg : app_adc_params_t , app_comp_params_t , app_i2c_params_t , app_i2s_params_t , app_pwm_params_t , app_qspi_params_t , app_spi_params_t , app_uart_params_t
- pin_group : dfu_uart_info_t
- pkc_done_callback : _hal_pkc_callback
- pkc_error_callback : _hal_pkc_callback
- pkc_msp_deinit : _hal_pkc_callback
- pkc_msp_init : _hal_pkc_callback
- pkc_overflow_callback : _hal_pkc_callback
- pnp_id : ble_dis_c_read_rsp_t
- positive_action : ancs_ntf_flags_t
- post_mode : _ll_rng_init , _rng_init
- power_lvl : gap_dev_adv_tx_power_t
- pre_existing : ancs_ntf_flags_t
- prescaler : _dual_timer_init , _ll_dual_timer_init , _ll_pwm_init_t
- present_mcu_mask : _keyram_mask
- present_xip_mask : _keyram_mask
- prev_ms : _calendar_handle
- previous_action : _iso7816_handle_t
- previous_state : _i2c_handle
- prf_buf : stack_heaps_table_t
- prim_cfg : gap_ext_adv_param_t
- priority : _dma_init , _ll_dma_init
- priv_mode : gap_ral_dev_info_t
- product_id : dis_c_pnp_id_t , dis_pnp_id_t
- product_version : dis_c_pnp_id_t , dis_pnp_id_t
- prog_delay : ble_sch_config_t
- prop : ble_gattc_char_t , gap_ext_adv_param_t , gap_ext_init_param_t , gap_ext_scan_param_t , gattc_browse_attr_char_t
- PRSquare : _ll_ecc_curve_init
- pub_ecdh_key : escs_eid_t
- pull : _aon_gpio_init , _gpio_init , _ll_aon_gpio_init , _ll_gpio_init , _ll_msio_init , _msio_init , app_gpiote_param_t , app_i2c_pin_t , app_i2s_pin_t , app_io_init_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t
- pulse_rate : bps_meas_t
- pulse_rate_present : bps_meas_t
- pwm_msp_deinit : _hal_pwm_callback
- pwm_msp_init : _hal_pwm_callback
- pwr_ble_ths : pwr_table_t
- pwr_delay_hslot : pwr_table_t
- pwr_delay_hus : pwr_table_t
- pwr_dur : pwr_table_t
- pwr_ext : pwr_table_t
- pwr_mgmt_app_timer_thrd : pwr_mgmt_var_box_t
- pwr_mgmt_ble_core_thrd : pwr_mgmt_var_box_t
- pwr_mgmt_rtc_timer_thrd : pwr_mgmt_var_box_t
- pwr_osc : pwr_table_t
- pwr_push_hus : pwr_table_t
- pwr_slp_elapsed_hander : _hal_pwr_handler
- pwr_timer_ths : pwr_table_t