gr55xx_ll_pkc.h
Go to the documentation of this file.
1
51 /* Define to prevent recursive inclusion -------------------------------------*/
52 #ifndef __GR55XX_LL_PKC_H__
53 #define __GR55XX_LL_PKC_H__
54
55 #ifdef __cplusplus
56 extern "C" {
57 #endif
58
59 /* Includes ------------------------------------------------------------------*/
60 #include "gr55xx.h"
61
62 #if defined (PKC)
63
68 /* Private macros ------------------------------------------------------------*/
72 #define ECC_U32_LENGTH (8)
73 #define RSA_U32_LENGTH (64)
83 /* Exported types ------------------------------------------------------------*/
84
91 typedef struct _ll_ecc_point
92 {
93 uint32_t X[ECC_U32_LENGTH];
95 uint32_t Y[ECC_U32_LENGTH];
97 } ll_ecc_point_t;
98
102 typedef struct _ll_ecc_curve_init
103 {
104 uint32_t A[ECC_U32_LENGTH];
105 uint32_t B[ECC_U32_LENGTH];
107 uint32_t P[ECC_U32_LENGTH];
108 uint32_t PRSquare[ECC_U32_LENGTH];
109 uint32_t ConstP;
111 uint32_t N[ECC_U32_LENGTH];
112 uint32_t NRSquare[ECC_U32_LENGTH];
113 uint32_t ConstN;
115 uint32_t H;
117 ll_ecc_point_t G;
119 } ll_ecc_curve_init_t;
120
124 typedef struct _ll_pkc_init
125 {
126 ll_ecc_curve_init_t *p_ecc_curve;
128 uint32_t data_bits;
130 } ll_pkc_init_t;
131
141 /* Exported constants --------------------------------------------------------*/
150 #define LL_PKC_WORKSTAT_BUSY PKC_WORKSTAT_BUSY
157 #define LL_PKC_INTEN_DONE PKC_INTEN_DONE
158 #define LL_PKC_INTEN_ERR PKC_INTEN_ERR
159 #define LL_PKC_INTEN_BAOVF PKC_INTEN_BAOVF
165 #define LL_PKC_BITS_LENGTH_MIN (256U)
166 #define LL_PKC_BITS_LENGTH_MAX (2048U)
167 #define LL_PKC_BIGMULTI_BITS_LENGTH_MAX (1024U)
173 #define LL_PKC_operation_mode_MULTIPLY (0x00000000U)
174 #define LL_PKC_operation_mode_INVERTION (1UL << PKC_SW_CTRL_OPMODE_Pos)
175 #define LL_PKC_operation_mode_ADD (2UL << PKC_SW_CTRL_OPMODE_Pos)
176 #define LL_PKC_operation_mode_SUB (3UL << PKC_SW_CTRL_OPMODE_Pos)
177 #define LL_PKC_operation_mode_COMPARE (4UL << PKC_SW_CTRL_OPMODE_Pos)
178 #define LL_PKC_operation_mode_LEFTSHIFT (5UL << PKC_SW_CTRL_OPMODE_Pos)
179 #define LL_PKC_operation_mode_BIGINTEGERMULTIPLY (6UL << PKC_SW_CTRL_OPMODE_Pos)
180 #define LL_PKC_operation_mode_BIGINTEGERADD (7UL << PKC_SW_CTRL_OPMODE_Pos)
190 #define LL_ECC_CURVE_DEFAULT_CONFIG LL_ECC_CURVE_SECP256R1_CONFIG
191
195 #define LL_ECC_CURVE_SECP256R1_CONFIG \
196 { \
197 .A = {0xFFFFFFFC, 0x00000004, 0x00000000, 0x00000000, 0x00000003, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFC}, \
198 .B = {0xDC30061D, 0x04874834, 0xE5A220AB, 0xF7212ED6, 0xACF005CD, 0x78843090, 0xD89CDF62, 0x29C4BDDF}, \
199 .P = {0xFFFFFFFF, 0x00000001, 0x00000000, 0x00000000, 0x00000000, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFF}, \
200 .PRSquare = {0x00000004, 0xFFFFFFFD, 0xFFFFFFFF, 0xFFFFFFFE, 0xFFFFFFFB, 0xFFFFFFFF, 0x00000000, 0x00000003}, \
201 .ConstP = 1, \
202 .N = {0xFFFFFFFF, 0x00000000, 0xFFFFFFFF, 0xFFFFFFFF, 0xBCE6FAAD, 0xA7179E84, 0xF3B9CAC2, 0xFC632551}, \
203 .NRSquare = {0x66E12D94, 0xF3D95620, 0x2845B239, 0x2B6BEC59, 0x4699799C, 0x49BD6FA6, 0x83244C95, 0xBE79EEA2}, \
204 .ConstN = 0xEE00BC4F, \
205 .H = 1, \
206 .G.X = {0x6B17D1F2, 0xE12C4247, 0xF8BCE6E5, 0x63A440F2, 0x77037D81, 0x2DEB33A0, 0xF4A13945, 0xD898C296}, \
207 .G.Y = {0x4FE342E2, 0xFE1A7F9B, 0x8EE7EB4A, 0x7C0F9E16, 0x2BCE3357, 0x6B315ECE, 0xCBB64068, 0x37BF51F5}, \
208 }
209
213 #define LL_ECC_CURVE_SECP256K1_CONFIG \
214 { \
215 .A = {0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000}, \
216 .B = {0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000007, 0x00001AB7}, \
217 .P = {0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFE, 0xFFFFFC2F}, \
218 .PRSquare = {0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000000, 0x00000001, 0x000007A2, 0x000E90A1}, \
219 .ConstP = 0XD2253531, \
220 .N = {0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFF, 0xFFFFFFFE, 0xBAAEDCE6, 0xAF48A03B, 0xBFD25E8C, 0xD0364141}, \
221 .NRSquare = {0x9D671CD5, 0x81C69BC5, 0xE697F5E4, 0x5BCD07C6, 0x741496C2, 0x0E7CF878, 0x896CF214, 0x67D7D140}, \
222 .ConstN = 0X5588B13F, \
223 .H = 1, \
224 .G.X = {0x79BE667E, 0xF9DCBBAC, 0x55A06295, 0xCE870B07, 0x029BFCDB, 0x2DCE28D9, 0x59F2815B, 0x16F81798}, \
225 .G.Y = {0x483ADA77, 0x26A3C465, 0x5DA4FBFC, 0x0E1108A8, 0xFD17B448, 0xA6855419, 0x9C47D08F, 0xFB10D4B8}, \
226 }
227
232 /* Exported macro ------------------------------------------------------------*/
248 #define LL_PKC_WriteReg(__INSTANCE__, __REG__, __VALUE__) WRITE_REG(__INSTANCE__->__REG__, (__VALUE__))
249
256 #define LL_PKC_ReadReg(__INSTANCE__, __REG__) READ_REG(__INSTANCE__->__REG__)
257
264 /* Exported functions --------------------------------------------------------*/
283 __STATIC_INLINE void ll_pkc_enable(pkc_regs_t *PKCx)
284 {
285 SET_BITS(PKCx->CTRL, PKC_CTRL_EN);
286 }
287
298 __STATIC_INLINE void ll_pkc_disable(pkc_regs_t *PKCx)
299 {
300 CLEAR_BITS(PKCx->CTRL, PKC_CTRL_EN);
301 }
302
313 __STATIC_INLINE uint32_t ll_pkc_is_enabled(pkc_regs_t *PKCx)
314 {
315 return (READ_BITS(PKCx->CTRL, PKC_CTRL_EN) == (PKC_CTRL_EN));
316 }
317
328 __STATIC_INLINE void ll_pkc_enable_hardware_start(pkc_regs_t *PKCx)
329 {
330 SET_BITS(PKCx->CTRL, PKC_CTRL_START);
331 }
332
343 __STATIC_INLINE void ll_pkc_disable_hardware_start(pkc_regs_t *PKCx)
344 {
345 CLEAR_BITS(PKCx->CTRL, PKC_CTRL_START);
346 }
347
358 __STATIC_INLINE uint32_t ll_pkc_is_enabled_hardware_start(pkc_regs_t *PKCx)
359 {
360 return (READ_BITS(PKCx->CTRL, PKC_CTRL_START) == (PKC_CTRL_START));
361 }
362
373 __STATIC_INLINE void ll_pkc_enable_software(pkc_regs_t *PKCx)
374 {
375 SET_BITS(PKCx->CTRL, PKC_CTRL_SWCTRL);
376 }
377
388 __STATIC_INLINE void ll_pkc_disable_software(pkc_regs_t *PKCx)
389 {
390 CLEAR_BITS(PKCx->CTRL, PKC_CTRL_SWCTRL);
391 }
392
403 __STATIC_INLINE uint32_t ll_pkc_is_enabled_software(pkc_regs_t *PKCx)
404 {
405 return (READ_BITS(PKCx->CTRL, PKC_CTRL_SWCTRL) == (PKC_CTRL_SWCTRL));
406 }
407
418 __STATIC_INLINE void ll_pkc_enable_reset(pkc_regs_t *PKCx)
419 {
420 SET_BITS(PKCx->CTRL, PKC_CTRL_SWRST);
421 }
422
433 __STATIC_INLINE void ll_pkc_disable_reset(pkc_regs_t *PKCx)
434 {
435 CLEAR_BITS(PKCx->CTRL, PKC_CTRL_SWRST);
436 }
437
448 __STATIC_INLINE uint32_t ll_pkc_is_enabled_reset(pkc_regs_t *PKCx)
449 {
450 return (READ_BITS(PKCx->CTRL, PKC_CTRL_SWRST) == (PKC_CTRL_SWRST));
451 }
452
464 __STATIC_INLINE void ll_pkc_set_k_pointer(pkc_regs_t *PKCx, uint32_t pointer)
465 {
466 MODIFY_REG(PKCx->CONFIG0, PKC_CONFIG0_KPTR, pointer << PKC_CONFIG0_KPTR_Pos);
467 }
468
479 __STATIC_INLINE uint32_t ll_pkc_get_k_pointer(pkc_regs_t *PKCx)
480 {
481 return (READ_BITS(PKCx->CONFIG0, PKC_CONFIG0_KPTR) >> PKC_CONFIG0_KPTR_Pos);
482 }
483
495 __STATIC_INLINE void ll_pkc_set_r_pointer(pkc_regs_t *PKCx, uint32_t pointer)
496 {
497 MODIFY_REG(PKCx->CONFIG0, PKC_CONFIG0_RPTR, pointer << PKC_CONFIG0_RPTR_Pos);
498 }
499
510 __STATIC_INLINE uint32_t ll_pkc_get_r_pointer(pkc_regs_t *PKCx)
511 {
512 return (READ_BITS(PKCx->CONFIG0, PKC_CONFIG0_RPTR) >> PKC_CONFIG0_RPTR_Pos);
513 }
514
526 __STATIC_INLINE void ll_pkc_set_p_pointer(pkc_regs_t *PKCx, uint32_t pointer)
527 {
528 MODIFY_REG(PKCx->CONFIG1, PKC_CONFIG1_PPTR, pointer << PKC_CONFIG1_PPTR_Pos);
529 }
530
541 __STATIC_INLINE uint32_t ll_pkc_get_p_pointer(pkc_regs_t *PKCx)
542 {
543 return (READ_BITS(PKCx->CONFIG1, PKC_CONFIG1_PPTR) >> PKC_CONFIG1_PPTR_Pos);
544 }
545
557 __STATIC_INLINE void ll_pkc_set_rsq_pointer(pkc_regs_t *PKCx, uint32_t pointer)
558 {
559 MODIFY_REG(PKCx->CONFIG1, PKC_CONFIG1_RSQPTR, pointer << PKC_CONFIG1_RSQPTR_Pos);
560 }
561
572 __STATIC_INLINE uint32_t ll_pkc_get_rsq_pointer(pkc_regs_t *PKCx)
573 {
574 return (READ_BITS(PKCx->CONFIG1, PKC_CONFIG1_RSQPTR) >> PKC_CONFIG1_RSQPTR_Pos);
575 }
576
588 __STATIC_INLINE void ll_pkc_set_gx_pointer(pkc_regs_t *PKCx, uint32_t pointer)
589 {
590 MODIFY_REG(PKCx->CONFIG2, PKC_CONFIG2_GXPTR, pointer << PKC_CONFIG2_GXPTR_Pos);
591 }
592
603 __STATIC_INLINE uint32_t ll_pkc_get_gx_pointer(pkc_regs_t *PKCx)
604 {
605 return (READ_BITS(PKCx->CONFIG2, PKC_CONFIG2_GXPTR) >> PKC_CONFIG2_GXPTR_Pos);
606 }
607
619 __STATIC_INLINE void ll_pkc_set_gy_pointer(pkc_regs_t *PKCx, uint32_t pointer)
620 {
621 MODIFY_REG(PKCx->CONFIG2, PKC_CONFIG2_GYPTR, pointer << PKC_CONFIG2_GYPTR_Pos);
622 }
623
634 __STATIC_INLINE uint32_t ll_pkc_get_gy_pointer(pkc_regs_t *PKCx)
635 {
636 return (READ_BITS(PKCx->CONFIG2, PKC_CONFIG2_GYPTR) >> PKC_CONFIG2_GYPTR_Pos);
637 }
638
650 __STATIC_INLINE void ll_pkc_set_gz_pointer(pkc_regs_t *PKCx, uint32_t pointer)
651 {
652 MODIFY_REG(PKCx->CONFIG3, PKC_CONFIG3_GZPTR, pointer << PKC_CONFIG3_GZPTR_Pos);
653 }
654
665 __STATIC_INLINE uint32_t ll_pkc_get_gz_pointer(pkc_regs_t *PKCx)
666 {
667 return (READ_BITS(PKCx->CONFIG3, PKC_CONFIG3_GZPTR) >> PKC_CONFIG3_GZPTR_Pos);
668 }
669
681 __STATIC_INLINE void ll_pkc_set_r0x_pointer(pkc_regs_t *PKCx, uint32_t pointer)
682 {
683 MODIFY_REG(PKCx->CONFIG3, PKC_CONFIG3_R0XPTR, pointer << PKC_CONFIG3_R0XPTR_Pos);
684 }
685
696 __STATIC_INLINE uint32_t ll_pkc_get_r0x_pointer(pkc_regs_t *PKCx)
697 {
698 return (READ_BITS(PKCx->CONFIG3, PKC_CONFIG3_R0XPTR) >> PKC_CONFIG3_R0XPTR_Pos);
699 }
700
712 __STATIC_INLINE void ll_pkc_set_r0y_pointer(pkc_regs_t *PKCx, uint32_t pointer)
713 {
714 MODIFY_REG(PKCx->CONFIG4, PKC_CONFIG4_R0YPTR, pointer << PKC_CONFIG4_R0YPTR_Pos);
715 }
716
727 __STATIC_INLINE uint32_t ll_pkc_get_r0y_pointer(pkc_regs_t *PKCx)
728 {
729 return (READ_BITS(PKCx->CONFIG4, PKC_CONFIG4_R0YPTR) >> PKC_CONFIG4_R0YPTR_Pos);
730 }
731
743 __STATIC_INLINE void ll_pkc_set_r0z_pointer(pkc_regs_t *PKCx, uint32_t pointer)
744 {
745 MODIFY_REG(PKCx->CONFIG4, PKC_CONFIG4_R0ZPTR, pointer << PKC_CONFIG4_R0ZPTR_Pos);
746 }
747
758 __STATIC_INLINE uint32_t ll_pkc_get_r0z_pointer(pkc_regs_t *PKCx)
759 {
760 return (READ_BITS(PKCx->CONFIG4, PKC_CONFIG4_R0ZPTR) >> PKC_CONFIG4_R0ZPTR_Pos);
761 }
762
774 __STATIC_INLINE void ll_pkc_set_r1x_pointer(pkc_regs_t *PKCx, uint32_t pointer)
775 {
776 MODIFY_REG(PKCx->CONFIG5, PKC_CONFIG5_R1XPTR, pointer << PKC_CONFIG5_R1XPTR_Pos);
777 }
778
789 __STATIC_INLINE uint32_t ll_pkc_get_r1x_pointer(pkc_regs_t *PKCx)
790 {
791 return (READ_BITS(PKCx->CONFIG5, PKC_CONFIG5_R1XPTR) >> PKC_CONFIG5_R1XPTR_Pos);
792 }
793
805 __STATIC_INLINE void ll_pkc_set_r1y_pointer(pkc_regs_t *PKCx, uint32_t pointer)
806 {
807 MODIFY_REG(PKCx->CONFIG5, PKC_CONFIG5_R1YPTR, pointer << PKC_CONFIG5_R1YPTR_Pos);
808 }
809
820 __STATIC_INLINE uint32_t ll_pkc_get_r1y_pointer(pkc_regs_t *PKCx)
821 {
822 return (READ_BITS(PKCx->CONFIG5, PKC_CONFIG5_R1YPTR) >> PKC_CONFIG5_R1YPTR_Pos);
823 }
824
836 __STATIC_INLINE void ll_pkc_set_r1z_pointer(pkc_regs_t *PKCx, uint32_t pointer)
837 {
838 MODIFY_REG(PKCx->CONFIG6, PKC_CONFIG6_R1ZPTR, pointer << PKC_CONFIG6_R1ZPTR_Pos);
839 }
840
851 __STATIC_INLINE uint32_t ll_pkc_get_r1z_pointer(pkc_regs_t *PKCx)
852 {
853 return (READ_BITS(PKCx->CONFIG6, PKC_CONFIG6_R1ZPTR) >> PKC_CONFIG6_R1ZPTR_Pos);
854 }
855
867 __STATIC_INLINE void ll_pkc_set_tmp1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
868 {
869 MODIFY_REG(PKCx->CONFIG6, PKC_CONFIG6_TMP1PTR, pointer << PKC_CONFIG6_TMP1PTR_Pos);
870 }
871
882 __STATIC_INLINE uint32_t ll_pkc_get_tmp1_pointer(pkc_regs_t *PKCx)
883 {
884 return (READ_BITS(PKCx->CONFIG6, PKC_CONFIG6_TMP1PTR) >> PKC_CONFIG6_TMP1PTR_Pos);
885 }
886
898 __STATIC_INLINE void ll_pkc_set_tmp2_pointer(pkc_regs_t *PKCx, uint32_t pointer)
899 {
900 MODIFY_REG(PKCx->CONFIG7, PKC_CONFIG7_TMP2PTR, pointer << PKC_CONFIG7_TMP2PTR_Pos);
901 }
902
913 __STATIC_INLINE uint32_t ll_pkc_get_tmp2_pointer(pkc_regs_t *PKCx)
914 {
915 return (READ_BITS(PKCx->CONFIG7, PKC_CONFIG7_TMP2PTR) >> PKC_CONFIG7_TMP2PTR_Pos);
916 }
917
929 __STATIC_INLINE void ll_pkc_set_tmp3_pointer(pkc_regs_t *PKCx, uint32_t pointer)
930 {
931 MODIFY_REG(PKCx->CONFIG7, PKC_CONFIG7_TMP3PTR, pointer << PKC_CONFIG7_TMP3PTR_Pos);
932 }
933
944 __STATIC_INLINE uint32_t ll_pkc_get_tmp3_pointer(pkc_regs_t *PKCx)
945 {
946 return (READ_BITS(PKCx->CONFIG7, PKC_CONFIG7_TMP3PTR) >> PKC_CONFIG7_TMP3PTR_Pos);
947 }
948
960 __STATIC_INLINE void ll_pkc_set_tmp4_pointer(pkc_regs_t *PKCx, uint32_t pointer)
961 {
962 MODIFY_REG(PKCx->CONFIG8, PKC_CONFIG8_TMP4PTR, pointer << PKC_CONFIG8_TMP4PTR_Pos);
963 }
964
975 __STATIC_INLINE uint32_t ll_pkc_get_tmp4_pointer(pkc_regs_t *PKCx)
976 {
977 return (READ_BITS(PKCx->CONFIG8, PKC_CONFIG8_TMP4PTR) >> PKC_CONFIG8_TMP4PTR_Pos);
978 }
979
991 __STATIC_INLINE void ll_pkc_set_tmp5_pointer(pkc_regs_t *PKCx, uint32_t pointer)
992 {
993 MODIFY_REG(PKCx->CONFIG8, PKC_CONFIG8_TMP5PTR, pointer << PKC_CONFIG8_TMP5PTR_Pos);
994 }
995
1006 __STATIC_INLINE uint32_t ll_pkc_get_tmp5_pointer(pkc_regs_t *PKCx)
1007 {
1008 return (READ_BITS(PKCx->CONFIG8, PKC_CONFIG8_TMP5PTR) >> PKC_CONFIG8_TMP5PTR_Pos);
1009 }
1010
1022 __STATIC_INLINE void ll_pkc_set_tmp6_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1023 {
1024 MODIFY_REG(PKCx->CONFIG9, PKC_CONFIG9_TMP6PTR, pointer << PKC_CONFIG9_TMP6PTR_Pos);
1025 }
1026
1037 __STATIC_INLINE uint32_t ll_pkc_get_tmp6_pointer(pkc_regs_t *PKCx)
1038 {
1039 return (READ_BITS(PKCx->CONFIG9, PKC_CONFIG9_TMP6PTR) >> PKC_CONFIG9_TMP6PTR_Pos);
1040 }
1041
1053 __STATIC_INLINE void ll_pkc_set_constant1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1054 {
1055 MODIFY_REG(PKCx->CONFIG9, PKC_CONFIG9_CONST1PTR, pointer << PKC_CONFIG9_CONST1PTR_Pos);
1056 }
1057
1068 __STATIC_INLINE uint32_t ll_pkc_get_constant1_pointer(pkc_regs_t *PKCx)
1069 {
1070 return (READ_BITS(PKCx->CONFIG9, PKC_CONFIG9_CONST1PTR) >> PKC_CONFIG9_CONST1PTR_Pos);
1071 }
1072
1084 __STATIC_INLINE void ll_pkc_set_x1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1085 {
1086 MODIFY_REG(PKCx->CONFIG10, PKC_CONFIG10_X1PTR, pointer << PKC_CONFIG10_X1PTR_Pos);
1087 }
1088
1099 __STATIC_INLINE uint32_t ll_pkc_get_x1_pointer(pkc_regs_t *PKCx)
1100 {
1101 return (READ_BITS(PKCx->CONFIG10, PKC_CONFIG10_X1PTR) >> PKC_CONFIG10_X1PTR_Pos);
1102 }
1103
1115 __STATIC_INLINE void ll_pkc_set_x2_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1116 {
1117 MODIFY_REG(PKCx->CONFIG10, PKC_CONFIG10_X2PTR, pointer << PKC_CONFIG10_X2PTR_Pos);
1118 }
1119
1130 __STATIC_INLINE uint32_t ll_pkc_get_x2_pointer(pkc_regs_t *PKCx)
1131 {
1132 return (READ_BITS(PKCx->CONFIG10, PKC_CONFIG10_X2PTR) >> PKC_CONFIG10_X2PTR_Pos);
1133 }
1134
1146 __STATIC_INLINE void ll_pkc_set_mitmp_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1147 {
1148 MODIFY_REG(PKCx->CONFIG11, PKC_CONFIG11_MITMPPTR, pointer << PKC_CONFIG11_MITMPPTR_Pos);
1149 }
1150
1161 __STATIC_INLINE uint32_t ll_pkc_get_mitmp_pointer(pkc_regs_t *PKCx)
1162 {
1163 return (READ_BITS(PKCx->CONFIG11, PKC_CONFIG11_MITMPPTR) >> PKC_CONFIG11_MITMPPTR_Pos);
1164 }
1165
1177 __STATIC_INLINE void ll_pkc_set_tmpk_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1178 {
1179 MODIFY_REG(PKCx->CONFIG11, PKC_CONFIG11_TMPKPTR, pointer << PKC_CONFIG11_TMPKPTR_Pos);
1180 }
1181
1192 __STATIC_INLINE uint32_t ll_pkc_get_tmpk_pointer(pkc_regs_t *PKCx)
1193 {
1194 return (READ_BITS(PKCx->CONFIG11, PKC_CONFIG11_TMPKPTR) >> PKC_CONFIG11_TMPKPTR_Pos);
1195 }
1196
1208 __STATIC_INLINE void ll_pkc_set_ecc_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1209 {
1210 MODIFY_REG(PKCx->CONFIG12, PKC_CONFIG12_APTR, pointer << PKC_CONFIG12_APTR_Pos);
1211 }
1212
1223 __STATIC_INLINE uint32_t ll_pkc_get_ecc_a_pointer(pkc_regs_t *PKCx)
1224 {
1225 return (READ_BITS(PKCx->CONFIG12, PKC_CONFIG12_APTR) >> PKC_CONFIG12_APTR_Pos);
1226 }
1227
1239 __STATIC_INLINE void ll_pkc_set_ecc_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1240 {
1241 MODIFY_REG(PKCx->CONFIG12, PKC_CONFIG12_BPTR, pointer << PKC_CONFIG12_BPTR_Pos);
1242 }
1243
1254 __STATIC_INLINE uint32_t ll_pkc_get_ecc_b_pointer(pkc_regs_t *PKCx)
1255 {
1256 return (READ_BITS(PKCx->CONFIG12, PKC_CONFIG12_BPTR) >> PKC_CONFIG12_BPTR_Pos);
1257 }
1258
1270 __STATIC_INLINE void ll_pkc_set_constp(pkc_regs_t *PKCx, uint32_t ConstP)
1271 {
1272 WRITE_REG(PKCx->CONFIG13, ConstP);
1273 }
1274
1285 __STATIC_INLINE uint32_t ll_pkc_get_constp(pkc_regs_t *PKCx)
1286 {
1287 return (READ_REG(PKCx->CONFIG13));
1288 }
1289
1300 __STATIC_INLINE void ll_pkc_enable_software_start(pkc_regs_t *PKCx)
1301 {
1302 SET_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_OPSTART);
1303 }
1304
1315 __STATIC_INLINE void ll_pkc_disable_software_start(pkc_regs_t *PKCx)
1316 {
1317 CLEAR_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_OPSTART);
1318 }
1319
1330 __STATIC_INLINE uint32_t ll_pkc_is_enabled_software_start(pkc_regs_t *PKCx)
1331 {
1332 return (READ_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_OPSTART) == (PKC_SW_CTRL_OPSTART));
1333 }
1334
1354 __STATIC_INLINE void ll_pkc_set_operation_mode(pkc_regs_t *PKCx, uint32_t operation_mode)
1355 {
1356 MODIFY_REG(PKCx->SW_CTRL, PKC_SW_CTRL_OPMODE, operation_mode);
1357 }
1358
1377 __STATIC_INLINE uint32_t ll_pkc_get_operation_mode(pkc_regs_t *PKCx)
1378 {
1379 return (READ_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_OPMODE));
1380 }
1381
1392 __STATIC_INLINE void ll_pkc_enable_dummy_multi(pkc_regs_t *PKCx)
1393 {
1394 SET_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_STARTDM);
1395 }
1396
1407 __STATIC_INLINE void ll_pkc_disable_dummy_multi(pkc_regs_t *PKCx)
1408 {
1409 CLEAR_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_STARTDM);
1410 }
1411
1422 __STATIC_INLINE uint32_t ll_pkc_is_enabled_dummy_multi(pkc_regs_t *PKCx)
1423 {
1424 return (READ_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_STARTDM) == (PKC_SW_CTRL_STARTDM));
1425 }
1426
1437 __STATIC_INLINE void ll_pkc_enable_random_clock_gating(pkc_regs_t *PKCx)
1438 {
1439 SET_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_RANDEN);
1440 }
1441
1452 __STATIC_INLINE void ll_pkc_disable_random_clock_gating(pkc_regs_t *PKCx)
1453 {
1454 CLEAR_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_RANDEN);
1455 }
1456
1467 __STATIC_INLINE uint32_t ll_pkc_is_enabled_random_clock_gating(pkc_regs_t *PKCx)
1468 {
1469 return (READ_BITS(PKCx->SW_CTRL, PKC_SW_CTRL_RANDEN) == (PKC_SW_CTRL_RANDEN));
1470 }
1471
1483 __STATIC_INLINE void ll_pkc_set_mm_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1484 {
1485 MODIFY_REG(PKCx->SW_CONFIG0, PKC_SW_CONFIG0_MMAPTR, pointer << PKC_SW_CONFIG0_MMAPTR_Pos);
1486 }
1487
1498 __STATIC_INLINE uint32_t ll_pkc_get_mm_a_pointer(pkc_regs_t *PKCx)
1499 {
1500 return (READ_BITS(PKCx->SW_CONFIG0, PKC_SW_CONFIG0_MMAPTR) >> PKC_SW_CONFIG0_MMAPTR_Pos);
1501 }
1502
1514 __STATIC_INLINE void ll_pkc_set_mm_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1515 {
1516 MODIFY_REG(PKCx->SW_CONFIG0, PKC_SW_CONFIG0_MMBPTR, pointer << PKC_SW_CONFIG0_MMBPTR_Pos);
1517 }
1518
1529 __STATIC_INLINE uint32_t ll_pkc_get_mm_b_pointer(pkc_regs_t *PKCx)
1530 {
1531 return (READ_BITS(PKCx->SW_CONFIG0, PKC_SW_CONFIG0_MMBPTR) >> PKC_SW_CONFIG0_MMBPTR_Pos);
1532 }
1533
1545 __STATIC_INLINE void ll_pkc_set_mm_p_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1546 {
1547 MODIFY_REG(PKCx->SW_CONFIG1, PKC_SW_CONFIG1_MMPPTR, pointer << PKC_SW_CONFIG1_MMPPTR_Pos);
1548 }
1549
1560 __STATIC_INLINE uint32_t ll_pkc_get_mm_p_pointer(pkc_regs_t *PKCx)
1561 {
1562 return (READ_BITS(PKCx->SW_CONFIG1, PKC_SW_CONFIG1_MMPPTR) >> PKC_SW_CONFIG1_MMPPTR_Pos);
1563 }
1564
1576 __STATIC_INLINE void ll_pkc_set_mm_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1577 {
1578 MODIFY_REG(PKCx->SW_CONFIG1, PKC_SW_CONFIG1_MMCPTR, pointer << PKC_SW_CONFIG1_MMCPTR_Pos);
1579 }
1580
1591 __STATIC_INLINE uint32_t ll_pkc_get_mm_c_pointer(pkc_regs_t *PKCx)
1592 {
1593 return (READ_BITS(PKCx->SW_CONFIG1, PKC_SW_CONFIG1_MMCPTR) >> PKC_SW_CONFIG1_MMCPTR_Pos);
1594 }
1595
1607 __STATIC_INLINE void ll_pkc_set_mas_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1608 {
1609 MODIFY_REG(PKCx->SW_CONFIG2, PKC_SW_CONFIG2_MASAPTR, pointer << PKC_SW_CONFIG2_MASAPTR_Pos);
1610 }
1611
1622 __STATIC_INLINE uint32_t ll_pkc_get_mas_a_pointer(pkc_regs_t *PKCx)
1623 {
1624 return (READ_BITS(PKCx->SW_CONFIG2, PKC_SW_CONFIG2_MASAPTR) >> PKC_SW_CONFIG2_MASAPTR_Pos);
1625 }
1626
1638 __STATIC_INLINE void ll_pkc_set_mas_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1639 {
1640 MODIFY_REG(PKCx->SW_CONFIG2, PKC_SW_CONFIG2_MASBPTR, pointer << PKC_SW_CONFIG2_MASBPTR_Pos);
1641 }
1642
1653 __STATIC_INLINE uint32_t ll_pkc_get_mas_b_pointer(pkc_regs_t *PKCx)
1654 {
1655 return (READ_BITS(PKCx->SW_CONFIG2, PKC_SW_CONFIG2_MASBPTR) >> PKC_SW_CONFIG2_MASBPTR_Pos);
1656 }
1657
1669 __STATIC_INLINE void ll_pkc_set_mas_p_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1670 {
1671 MODIFY_REG(PKCx->SW_CONFIG3, PKC_SW_CONFIG3_MASPPTR, pointer << PKC_SW_CONFIG3_MASPPTR_Pos);
1672 }
1673
1684 __STATIC_INLINE uint32_t ll_pkc_get_mas_p_pointer(pkc_regs_t *PKCx)
1685 {
1686 return (READ_BITS(PKCx->SW_CONFIG3, PKC_SW_CONFIG3_MASPPTR) >> PKC_SW_CONFIG3_MASPPTR_Pos);
1687 }
1688
1700 __STATIC_INLINE void ll_pkc_set_mas_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1701 {
1702 MODIFY_REG(PKCx->SW_CONFIG3, PKC_SW_CONFIG3_MASCPTR, pointer << PKC_SW_CONFIG3_MASCPTR_Pos);
1703 }
1704
1715 __STATIC_INLINE uint32_t ll_pkc_get_mas_c_pointer(pkc_regs_t *PKCx)
1716 {
1717 return (READ_BITS(PKCx->SW_CONFIG3, PKC_SW_CONFIG3_MASCPTR) >> PKC_SW_CONFIG3_MASCPTR_Pos);
1718 }
1719
1731 __STATIC_INLINE void ll_pkc_set_mi_u_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1732 {
1733 MODIFY_REG(PKCx->SW_CONFIG4, PKC_SW_CONFIG4_MIUPTR, pointer << PKC_SW_CONFIG4_MIUPTR_Pos);
1734 }
1735
1746 __STATIC_INLINE uint32_t ll_pkc_get_mi_u_pointer(pkc_regs_t *PKCx)
1747 {
1748 return (READ_BITS(PKCx->SW_CONFIG4, PKC_SW_CONFIG4_MIUPTR) >> PKC_SW_CONFIG4_MIUPTR_Pos);
1749 }
1750
1762 __STATIC_INLINE void ll_pkc_set_mi_v_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1763 {
1764 MODIFY_REG(PKCx->SW_CONFIG4, PKC_SW_CONFIG4_MIVPTR, pointer << PKC_SW_CONFIG4_MIVPTR_Pos);
1765 }
1766
1777 __STATIC_INLINE uint32_t ll_pkc_get_mi_v_pointer(pkc_regs_t *PKCx)
1778 {
1779 return (READ_BITS(PKCx->SW_CONFIG4, PKC_SW_CONFIG4_MIVPTR) >> PKC_SW_CONFIG4_MIVPTR_Pos);
1780 }
1781
1793 __STATIC_INLINE void ll_pkc_set_mi_x1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1794 {
1795 MODIFY_REG(PKCx->SW_CONFIG5, PKC_SW_CONFIG5_MIX1PTR, pointer << PKC_SW_CONFIG5_MIX1PTR_Pos);
1796 }
1797
1808 __STATIC_INLINE uint32_t ll_pkc_get_mi_x1_pointer(pkc_regs_t *PKCx)
1809 {
1810 return (READ_BITS(PKCx->SW_CONFIG5, PKC_SW_CONFIG5_MIX1PTR) >> PKC_SW_CONFIG5_MIX1PTR_Pos);
1811 }
1812
1824 __STATIC_INLINE void ll_pkc_set_mi_x2_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1825 {
1826 MODIFY_REG(PKCx->SW_CONFIG5, PKC_SW_CONFIG5_MIX2PTR, pointer << PKC_SW_CONFIG5_MIX2PTR_Pos);
1827 }
1828
1839 __STATIC_INLINE uint32_t ll_pkc_get_mi_x2_pointer(pkc_regs_t *PKCx)
1840 {
1841 return (READ_BITS(PKCx->SW_CONFIG5, PKC_SW_CONFIG5_MIX2PTR) >> PKC_SW_CONFIG5_MIX2PTR_Pos);
1842 }
1843
1855 __STATIC_INLINE void ll_pkc_set_swmi_tmp_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1856 {
1857 MODIFY_REG(PKCx->SW_CONFIG6, PKC_SW_CONFIG6_MITMPPTR, pointer << PKC_SW_CONFIG6_MITMPPTR_Pos);
1858 }
1859
1870 __STATIC_INLINE uint32_t ll_pkc_get_swmi_tmp_pointer(pkc_regs_t *PKCx)
1871 {
1872 return (READ_BITS(PKCx->SW_CONFIG6, PKC_SW_CONFIG6_MITMPPTR) >> PKC_SW_CONFIG6_MITMPPTR_Pos);
1873 }
1874
1886 __STATIC_INLINE void ll_pkc_set_operation_word_length(pkc_regs_t *PKCx, uint32_t WordLength)
1887 {
1888 MODIFY_REG(PKCx->SW_CONFIG7, PKC_SW_CONFIG7_WORDLEN, (WordLength >> 5) - 1);
1889 }
1890
1901 __STATIC_INLINE uint32_t ll_pkc_get_operation_word_length(pkc_regs_t *PKCx)
1902 {
1903 return ((READ_BITS(PKCx->SW_CONFIG7, PKC_SW_CONFIG7_WORDLEN) + 1) << 5);
1904 }
1905
1916 __STATIC_INLINE uint32_t ll_pkc_get_mik_output(pkc_regs_t *PKCx)
1917 {
1918 return (READ_REG(PKCx->SW_CONFIG8) & PKC_SW_CONFIG8_MIKOUT_Msk);
1919 }
1920
1932 __STATIC_INLINE void ll_pkc_set_dummy_multiply_seed(pkc_regs_t *PKCx, uint32_t seed)
1933 {
1934 WRITE_REG(PKCx->SW_CONFIG9, seed);
1935 }
1936
1947 __STATIC_INLINE uint32_t ll_pkc_get_dummy_multiply_seed(pkc_regs_t *PKCx)
1948 {
1949 return (READ_REG(PKCx->SW_CONFIG9));
1950 }
1951
1963 __STATIC_INLINE void ll_pkc_set_bm_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1964 {
1965 MODIFY_REG(PKCx->SW_CONFIG10, PKC_SW_CONFIG10_BMAPTR, pointer << PKC_SW_CONFIG10_BMAPTR_Pos);
1966 }
1967
1978 __STATIC_INLINE uint32_t ll_pkc_get_bm_a_pointer(pkc_regs_t *PKCx)
1979 {
1980 return (READ_BITS(PKCx->SW_CONFIG10, PKC_SW_CONFIG10_BMAPTR) >> PKC_SW_CONFIG10_BMAPTR_Pos);
1981 }
1982
1994 __STATIC_INLINE void ll_pkc_set_bm_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
1995 {
1996 MODIFY_REG(PKCx->SW_CONFIG10, PKC_SW_CONFIG10_BMBPTR, pointer << PKC_SW_CONFIG10_BMBPTR_Pos);
1997 }
1998
2009 __STATIC_INLINE uint32_t ll_pkc_get_bm_b_pointer(pkc_regs_t *PKCx)
2010 {
2011 return (READ_BITS(PKCx->SW_CONFIG10, PKC_SW_CONFIG10_BMBPTR) >> PKC_SW_CONFIG10_BMBPTR_Pos);
2012 }
2013
2025 __STATIC_INLINE void ll_pkc_set_bm_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
2026 {
2027 MODIFY_REG(PKCx->SW_CONFIG11, PKC_SW_CONFIG11_BMCPTR, pointer << PKC_SW_CONFIG11_BMCPTR_Pos);
2028 }
2029
2040 __STATIC_INLINE uint32_t ll_pkc_get_bm_c_pointer(pkc_regs_t *PKCx)
2041 {
2042 return (READ_BITS(PKCx->SW_CONFIG11, PKC_SW_CONFIG11_BMCPTR) >> PKC_SW_CONFIG11_BMCPTR_Pos);
2043 }
2044
2056 __STATIC_INLINE void ll_pkc_set_ba_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
2057 {
2058 MODIFY_REG(PKCx->SW_CONFIG11, PKC_SW_CONFIG11_BAAPTR, pointer << PKC_SW_CONFIG11_BAAPTR_Pos);
2059 }
2060
2071 __STATIC_INLINE uint32_t ll_pkc_get_ba_a_pointer(pkc_regs_t *PKCx)
2072 {
2073 return (READ_BITS(PKCx->SW_CONFIG11, PKC_SW_CONFIG11_BAAPTR) >> PKC_SW_CONFIG11_BAAPTR_Pos);
2074 }
2075
2087 __STATIC_INLINE void ll_pkc_set_ba_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
2088 {
2089 MODIFY_REG(PKCx->SW_CONFIG12, PKC_SW_CONFIG12_BABPTR, pointer << PKC_SW_CONFIG12_BABPTR_Pos);
2090 }
2091
2102 __STATIC_INLINE uint32_t ll_pkc_get_ba_b_pointer(pkc_regs_t *PKCx)
2103 {
2104 return (READ_BITS(PKCx->SW_CONFIG12, PKC_SW_CONFIG12_BABPTR) >> PKC_SW_CONFIG12_BABPTR_Pos);
2105 }
2106
2118 __STATIC_INLINE void ll_pkc_set_ba_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
2119 {
2120 MODIFY_REG(PKCx->SW_CONFIG12, PKC_SW_CONFIG12_BACPTR, pointer << PKC_SW_CONFIG12_BACPTR_Pos);
2121 }
2122
2133 __STATIC_INLINE uint32_t ll_pkc_get_ba_c_pointer(pkc_regs_t *PKCx)
2134 {
2135 return (READ_BITS(PKCx->SW_CONFIG12, PKC_SW_CONFIG12_BACPTR) >> PKC_SW_CONFIG12_BACPTR_Pos);
2136 }
2137
2149 __STATIC_INLINE void ll_pkc_set_random_clock_gating_seed(pkc_regs_t *PKCx, uint32_t seed)
2150 {
2151 WRITE_REG(PKCx->SW_CONFIG13, seed);
2152 }
2153
2164 __STATIC_INLINE uint32_t ll_pkc_get_random_clock_gating_seed(pkc_regs_t *PKCx)
2165 {
2166 return (READ_REG(PKCx->SW_CONFIG13));
2167 }
2168
2185 __STATIC_INLINE void ll_pkc_enable_it_done(pkc_regs_t *PKCx)
2186 {
2187 SET_BITS(PKCx->INTEN, PKC_INTEN_DONE);
2188 }
2189
2200 __STATIC_INLINE void ll_pkc_enable_it_err(pkc_regs_t *PKCx)
2201 {
2202 SET_BITS(PKCx->INTEN, PKC_INTEN_ERR);
2203 }
2204
2215 __STATIC_INLINE void ll_pkc_enable_it_big_add_overflow(pkc_regs_t *PKCx)
2216 {
2217 SET_BITS(PKCx->INTEN, PKC_INTEN_BAOVF);
2218 }
2219
2230 __STATIC_INLINE void ll_pkc_disable_it_done(pkc_regs_t *PKCx)
2231 {
2232 CLEAR_BITS(PKCx->INTEN, PKC_INTEN_DONE);
2233 }
2234
2245 __STATIC_INLINE void ll_pkc_disable_it_err(pkc_regs_t *PKCx)
2246 {
2247 CLEAR_BITS(PKCx->INTEN, PKC_INTEN_ERR);
2248 }
2249
2260 __STATIC_INLINE void ll_pkc_disable_it_big_add_overflow(pkc_regs_t *PKCx)
2261 {
2262 CLEAR_BITS(PKCx->INTEN, PKC_INTEN_BAOVF);
2263 }
2264
2275 __STATIC_INLINE uint32_t ll_pkc_is_enable_it_done(pkc_regs_t *PKCx)
2276 {
2277 return (READ_BITS(PKCx->INTEN, PKC_INTEN_DONE) == PKC_INTEN_DONE);
2278 }
2279
2290 __STATIC_INLINE uint32_t ll_pkc_is_enable_it_err(pkc_regs_t *PKCx)
2291 {
2292 return (READ_BITS(PKCx->INTEN, PKC_INTEN_ERR) == PKC_INTEN_ERR);
2293 }
2294
2305 __STATIC_INLINE uint32_t ll_pkc_is_enable_it_big_add_overflow(pkc_regs_t *PKCx)
2306 {
2307 return (READ_BITS(PKCx->INTEN, PKC_INTEN_BAOVF) == PKC_INTEN_BAOVF);
2308 }
2309
2326 __STATIC_INLINE uint32_t ll_pkc_is_action_flag_it_done(pkc_regs_t *PKCx)
2327 {
2328 return (READ_BITS(PKCx->INTSTAT, PKC_INTSTAT_DONE) == PKC_INTSTAT_DONE);
2329 }
2330
2341 __STATIC_INLINE uint32_t ll_pkc_is_action_flag_it_err(pkc_regs_t *PKCx)
2342 {
2343 return (READ_BITS(PKCx->INTSTAT, PKC_INTSTAT_ERR) == PKC_INTSTAT_ERR);
2344 }
2345
2356 __STATIC_INLINE uint32_t ll_pkc_is_action_flag_it_big_add_overflow(pkc_regs_t *PKCx)
2357 {
2358 return (READ_BITS(PKCx->INTSTAT, PKC_INTSTAT_BAOVF) == PKC_INTSTAT_BAOVF);
2359 }
2360
2371 __STATIC_INLINE void ll_pkc_clear_flag_it_done(pkc_regs_t *PKCx)
2372 {
2373 SET_BITS(PKCx->INTSTAT, PKC_INTSTAT_DONE);
2374 }
2375
2386 __STATIC_INLINE void ll_pkc_clear_flag_it_err(pkc_regs_t *PKCx)
2387 {
2388 SET_BITS(PKCx->INTSTAT, PKC_INTSTAT_ERR);
2389 }
2390
2401 __STATIC_INLINE void ll_pkc_clear_flag_it_big_add_overflow(pkc_regs_t *PKCx)
2402 {
2403 SET_BITS(PKCx->INTSTAT, PKC_INTSTAT_BAOVF);
2404 }
2405
2416 __STATIC_INLINE uint32_t ll_pkc_is_action_flag_busy(pkc_regs_t *PKCx)
2417 {
2418 return (READ_BITS(PKCx->WORKSTAT, PKC_WORKSTAT_BUSY) == PKC_WORKSTAT_BUSY);
2419 }
2420
2434 error_status_t ll_pkc_deinit(pkc_regs_t *PKCx);
2435
2446 error_status_t ll_pkc_init(pkc_regs_t *PKCx, ll_pkc_init_t *p_pkc_init);
2447
2454 void ll_pkc_struct_init(ll_pkc_init_t *p_pkc_init);
2455
2460 #endif /* PKC */
2461
2462 #ifdef __cplusplus
2463 }
2464 #endif
2465
2466 #endif /* __GR55XX_LL_PKC_H__ */
2467
ll_pkc_is_enabled_hardware_start
__STATIC_INLINE uint32_t ll_pkc_is_enabled_hardware_start(pkc_regs_t *PKCx)
Indicate whether the pkc start in hardware mode is enabled.
Definition: gr55xx_ll_pkc.h:358
ll_pkc_enable_it_err
__STATIC_INLINE void ll_pkc_enable_it_err(pkc_regs_t *PKCx)
Enable the operation error interrupt.
Definition: gr55xx_ll_pkc.h:2200
ll_pkc_get_bm_a_pointer
__STATIC_INLINE uint32_t ll_pkc_get_bm_a_pointer(pkc_regs_t *PKCx)
Get big integer operand A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1978
ll_pkc_get_tmp6_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmp6_pointer(pkc_regs_t *PKCx)
Get PKC parameter Tmp6 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1037
ll_pkc_set_k_pointer
__STATIC_INLINE void ll_pkc_set_k_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter k pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:464
ll_pkc_get_tmp1_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmp1_pointer(pkc_regs_t *PKCx)
Get PKC parameter Tmp1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:882
ll_pkc_set_tmpk_pointer
__STATIC_INLINE void ll_pkc_set_tmpk_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter TmpK pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1177
ll_pkc_get_gy_pointer
__STATIC_INLINE uint32_t ll_pkc_get_gy_pointer(pkc_regs_t *PKCx)
Get PKC parameter Gy pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:634
ll_pkc_disable_software
__STATIC_INLINE void ll_pkc_disable_software(pkc_regs_t *PKCx)
Disable pkc software mode.
Definition: gr55xx_ll_pkc.h:388
ll_pkc_get_tmpk_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmpk_pointer(pkc_regs_t *PKCx)
Get PKC parameter TmpK pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1192
ll_pkc_get_random_clock_gating_seed
__STATIC_INLINE uint32_t ll_pkc_get_random_clock_gating_seed(pkc_regs_t *PKCx)
Get random clock gating seed.
Definition: gr55xx_ll_pkc.h:2164
ll_pkc_is_enabled
__STATIC_INLINE uint32_t ll_pkc_is_enabled(pkc_regs_t *PKCx)
Indicate whether the pkc is enabled.
Definition: gr55xx_ll_pkc.h:313
ll_pkc_get_p_pointer
__STATIC_INLINE uint32_t ll_pkc_get_p_pointer(pkc_regs_t *PKCx)
Get PKC parameter p pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:541
ll_pkc_get_gx_pointer
__STATIC_INLINE uint32_t ll_pkc_get_gx_pointer(pkc_regs_t *PKCx)
Get PKC parameter Gx pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:603
ll_pkc_clear_flag_it_done
__STATIC_INLINE void ll_pkc_clear_flag_it_done(pkc_regs_t *PKCx)
Clear the operation done interrupt flag.
Definition: gr55xx_ll_pkc.h:2371
ll_pkc_set_mm_a_pointer
__STATIC_INLINE void ll_pkc_set_mm_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular multiplication parameter A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1483
ll_pkc_init
error_status_t ll_pkc_init(pkc_regs_t *PKCx, ll_pkc_init_t *p_pkc_init)
Initialize PKC registers according to the specified parameters in p_pkc_init.
ll_pkc_set_mi_x1_pointer
__STATIC_INLINE void ll_pkc_set_mi_x1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular invertion parameter X1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1793
ll_pkc_set_operation_word_length
__STATIC_INLINE void ll_pkc_set_operation_word_length(pkc_regs_t *PKCx, uint32_t WordLength)
Set operation word length-bits.
Definition: gr55xx_ll_pkc.h:1886
ll_pkc_get_r0z_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r0z_pointer(pkc_regs_t *PKCx)
Get PKC parameter R0z pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:758
ll_pkc_get_mitmp_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mitmp_pointer(pkc_regs_t *PKCx)
Get PKC parameter MITmp pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1161
ll_pkc_set_mitmp_pointer
__STATIC_INLINE void ll_pkc_set_mitmp_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter MITmp pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1146
ll_pkc_get_mm_a_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mm_a_pointer(pkc_regs_t *PKCx)
Get modular multiplication parameter A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1498
ll_pkc_set_gx_pointer
__STATIC_INLINE void ll_pkc_set_gx_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Gx pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:588
ll_pkc_get_constp
__STATIC_INLINE uint32_t ll_pkc_get_constp(pkc_regs_t *PKCx)
Get constant value for montgomery multiply in pkc sram.
Definition: gr55xx_ll_pkc.h:1285
ll_pkc_set_r_pointer
__STATIC_INLINE void ll_pkc_set_r_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter r pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:495
ll_ecc_curve_init_t
struct _ll_ecc_curve_init ll_ecc_curve_init_t
LL PKC ECC P-256 Elliptic Curve Init Structure definition.
ll_pkc_get_rsq_pointer
__STATIC_INLINE uint32_t ll_pkc_get_rsq_pointer(pkc_regs_t *PKCx)
Get PKC parameter R^2 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:572
ll_pkc_enable_dummy_multi
__STATIC_INLINE void ll_pkc_enable_dummy_multi(pkc_regs_t *PKCx)
Enable Dummy Multi in software mode.
Definition: gr55xx_ll_pkc.h:1392
ll_pkc_is_enabled_reset
__STATIC_INLINE uint32_t ll_pkc_is_enabled_reset(pkc_regs_t *PKCx)
Indicate whether the pkc reset is enabled.
Definition: gr55xx_ll_pkc.h:448
ll_pkc_disable_random_clock_gating
__STATIC_INLINE void ll_pkc_disable_random_clock_gating(pkc_regs_t *PKCx)
Disable Random Clock Gating in software mode.
Definition: gr55xx_ll_pkc.h:1452
ll_pkc_set_mm_b_pointer
__STATIC_INLINE void ll_pkc_set_mm_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular multiplication parameter B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1514
ll_pkc_set_mas_p_pointer
__STATIC_INLINE void ll_pkc_set_mas_p_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular add/sub parameter P pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1669
ll_pkc_get_r1z_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r1z_pointer(pkc_regs_t *PKCx)
Get PKC parameter R1z pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:851
ll_pkc_get_tmp2_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmp2_pointer(pkc_regs_t *PKCx)
Get PKC parameter Tmp2 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:913
ll_pkc_get_mi_x2_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mi_x2_pointer(pkc_regs_t *PKCx)
Get modular invertion parameter X1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1839
ll_pkc_set_r1z_pointer
__STATIC_INLINE void ll_pkc_set_r1z_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R1z pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:836
ll_pkc_get_ba_c_pointer
__STATIC_INLINE uint32_t ll_pkc_get_ba_c_pointer(pkc_regs_t *PKCx)
Get big integer result C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2133
_ll_pkc_init::p_ecc_curve
ll_ecc_curve_init_t * p_ecc_curve
Definition: gr55xx_ll_pkc.h:126
_ll_ecc_curve_init::A
uint32_t A[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:104
ll_pkc_set_bm_a_pointer
__STATIC_INLINE void ll_pkc_set_bm_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set big integer operand A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1963
ll_pkc_is_enable_it_big_add_overflow
__STATIC_INLINE uint32_t ll_pkc_is_enable_it_big_add_overflow(pkc_regs_t *PKCx)
Indicate whether the big integer overflow interrupt is enable.
Definition: gr55xx_ll_pkc.h:2305
ll_pkc_get_mas_b_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mas_b_pointer(pkc_regs_t *PKCx)
Get modular add/sub parameter B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1653
ll_pkc_disable_it_big_add_overflow
__STATIC_INLINE void ll_pkc_disable_it_big_add_overflow(pkc_regs_t *PKCx)
Disable the big integer overflow interrupt.
Definition: gr55xx_ll_pkc.h:2260
ll_pkc_set_x1_pointer
__STATIC_INLINE void ll_pkc_set_x1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter X1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1084
ll_pkc_enable_software_start
__STATIC_INLINE void ll_pkc_enable_software_start(pkc_regs_t *PKCx)
Enable pkc start in software mode.
Definition: gr55xx_ll_pkc.h:1300
ll_pkc_set_mm_c_pointer
__STATIC_INLINE void ll_pkc_set_mm_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular multiplication parameter C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1576
_ll_pkc_init::data_bits
uint32_t data_bits
Definition: gr55xx_ll_pkc.h:128
ll_pkc_set_ecc_b_pointer
__STATIC_INLINE void ll_pkc_set_ecc_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set ECC parameter B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1239
ll_pkc_set_mas_c_pointer
__STATIC_INLINE void ll_pkc_set_mas_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular add/sub parameter C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1700
ll_pkc_get_r1y_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r1y_pointer(pkc_regs_t *PKCx)
Get PKC parameter R1y pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:820
ll_pkc_get_r0y_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r0y_pointer(pkc_regs_t *PKCx)
Get PKC parameter R0y pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:727
ll_pkc_set_mi_v_pointer
__STATIC_INLINE void ll_pkc_set_mi_v_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular invertion parameter V pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1762
ll_pkc_get_bm_b_pointer
__STATIC_INLINE uint32_t ll_pkc_get_bm_b_pointer(pkc_regs_t *PKCx)
Get big integer operand B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2009
_ll_ecc_curve_init
LL PKC ECC P-256 Elliptic Curve Init Structure definition.
Definition: gr55xx_ll_pkc.h:103
_ll_pkc_init
LL PKC Init Structure definition.
Definition: gr55xx_ll_pkc.h:125
ll_pkc_set_x2_pointer
__STATIC_INLINE void ll_pkc_set_x2_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter X2 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1115
ll_pkc_is_action_flag_busy
__STATIC_INLINE uint32_t ll_pkc_is_action_flag_busy(pkc_regs_t *PKCx)
Indicate whether the busy flag is set.
Definition: gr55xx_ll_pkc.h:2416
ll_pkc_get_gz_pointer
__STATIC_INLINE uint32_t ll_pkc_get_gz_pointer(pkc_regs_t *PKCx)
Get PKC parameter Gz pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:665
ll_pkc_set_r1y_pointer
__STATIC_INLINE void ll_pkc_set_r1y_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R1y pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:805
ll_pkc_set_random_clock_gating_seed
__STATIC_INLINE void ll_pkc_set_random_clock_gating_seed(pkc_regs_t *PKCx, uint32_t seed)
Set random clock gating seed.
Definition: gr55xx_ll_pkc.h:2149
_ll_ecc_curve_init::PRSquare
uint32_t PRSquare[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:108
ll_pkc_disable_it_done
__STATIC_INLINE void ll_pkc_disable_it_done(pkc_regs_t *PKCx)
Disable the operation done interrupt.
Definition: gr55xx_ll_pkc.h:2230
ll_pkc_set_swmi_tmp_pointer
__STATIC_INLINE void ll_pkc_set_swmi_tmp_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular invertion parameter Tmp pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1855
ll_pkc_get_mas_c_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mas_c_pointer(pkc_regs_t *PKCx)
Get modular add/sub parameter C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1715
ll_pkc_get_operation_word_length
__STATIC_INLINE uint32_t ll_pkc_get_operation_word_length(pkc_regs_t *PKCx)
Get operation word length-bits.
Definition: gr55xx_ll_pkc.h:1901
ll_pkc_get_mm_c_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mm_c_pointer(pkc_regs_t *PKCx)
Get modular multiplication parameter C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1591
ll_pkc_get_mas_p_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mas_p_pointer(pkc_regs_t *PKCx)
Get modular add/sub parameter P pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1684
ll_pkc_is_action_flag_it_big_add_overflow
__STATIC_INLINE uint32_t ll_pkc_is_action_flag_it_big_add_overflow(pkc_regs_t *PKCx)
Indicate whether the big integer overflow interrupt is pending.
Definition: gr55xx_ll_pkc.h:2356
_ll_ecc_curve_init::H
uint32_t H
Definition: gr55xx_ll_pkc.h:115
ll_pkc_set_r1x_pointer
__STATIC_INLINE void ll_pkc_set_r1x_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R1x pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:774
ll_pkc_set_tmp1_pointer
__STATIC_INLINE void ll_pkc_set_tmp1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Tmp1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:867
ll_pkc_set_tmp4_pointer
__STATIC_INLINE void ll_pkc_set_tmp4_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Tmp4 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:960
ll_pkc_set_tmp2_pointer
__STATIC_INLINE void ll_pkc_set_tmp2_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Tmp2 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:898
ll_pkc_set_constant1_pointer
__STATIC_INLINE void ll_pkc_set_constant1_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Constant1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1053
ll_pkc_get_ecc_b_pointer
__STATIC_INLINE uint32_t ll_pkc_get_ecc_b_pointer(pkc_regs_t *PKCx)
Get ECC parameter B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1254
_ll_ecc_curve_init::ConstP
uint32_t ConstP
Definition: gr55xx_ll_pkc.h:109
ll_pkc_set_mm_p_pointer
__STATIC_INLINE void ll_pkc_set_mm_p_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular multiplication parameter P pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1545
ll_pkc_get_mm_b_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mm_b_pointer(pkc_regs_t *PKCx)
Get modular multiplication parameter B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1529
ll_pkc_get_r_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r_pointer(pkc_regs_t *PKCx)
Get PKC parameter r pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:510
ll_pkc_get_tmp4_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmp4_pointer(pkc_regs_t *PKCx)
Get PKC parameter Tmp4 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:975
ll_pkc_disable_reset
__STATIC_INLINE void ll_pkc_disable_reset(pkc_regs_t *PKCx)
Disable pkc reset.
Definition: gr55xx_ll_pkc.h:433
ll_pkc_set_mi_x2_pointer
__STATIC_INLINE void ll_pkc_set_mi_x2_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular invertion parameter X1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1824
ll_pkc_enable
__STATIC_INLINE void ll_pkc_enable(pkc_regs_t *PKCx)
Enable pkc.
Definition: gr55xx_ll_pkc.h:283
ll_pkc_get_operation_mode
__STATIC_INLINE uint32_t ll_pkc_get_operation_mode(pkc_regs_t *PKCx)
Get operation mode in software mode.
Definition: gr55xx_ll_pkc.h:1377
_ll_ecc_curve_init::P
uint32_t P[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:107
ll_pkc_get_ba_a_pointer
__STATIC_INLINE uint32_t ll_pkc_get_ba_a_pointer(pkc_regs_t *PKCx)
Get big integer operand A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2071
ll_pkc_is_action_flag_it_done
__STATIC_INLINE uint32_t ll_pkc_is_action_flag_it_done(pkc_regs_t *PKCx)
Indicate whether the operation done interrupt is pending.
Definition: gr55xx_ll_pkc.h:2326
ll_pkc_clear_flag_it_err
__STATIC_INLINE void ll_pkc_clear_flag_it_err(pkc_regs_t *PKCx)
Clear the operation error interrupt flag.
Definition: gr55xx_ll_pkc.h:2386
_ll_ecc_point
LL PKC ECC Point Structure definition.
Definition: gr55xx_ll_pkc.h:92
ll_pkc_get_bm_c_pointer
__STATIC_INLINE uint32_t ll_pkc_get_bm_c_pointer(pkc_regs_t *PKCx)
Get big integer result C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2040
_ll_ecc_curve_init::NRSquare
uint32_t NRSquare[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:112
ll_pkc_set_tmp5_pointer
__STATIC_INLINE void ll_pkc_set_tmp5_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Tmp5 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:991
ll_pkc_set_dummy_multiply_seed
__STATIC_INLINE void ll_pkc_set_dummy_multiply_seed(pkc_regs_t *PKCx, uint32_t seed)
Set dummy multiply seed.
Definition: gr55xx_ll_pkc.h:1932
ECC_U32_LENGTH
#define ECC_U32_LENGTH
Definition: gr55xx_ll_pkc.h:72
ll_pkc_set_ba_c_pointer
__STATIC_INLINE void ll_pkc_set_ba_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set big integer result C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2118
ll_pkc_get_mi_x1_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mi_x1_pointer(pkc_regs_t *PKCx)
Get modular invertion parameter X1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1808
ll_pkc_set_bm_c_pointer
__STATIC_INLINE void ll_pkc_set_bm_c_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set big integer result C pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2025
ll_pkc_set_r0x_pointer
__STATIC_INLINE void ll_pkc_set_r0x_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R0x pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:681
ll_pkc_is_enabled_dummy_multi
__STATIC_INLINE uint32_t ll_pkc_is_enabled_dummy_multi(pkc_regs_t *PKCx)
Indicate whether the Dummy Multi in software mode is enabled.
Definition: gr55xx_ll_pkc.h:1422
ll_pkc_disable
__STATIC_INLINE void ll_pkc_disable(pkc_regs_t *PKCx)
Disable pkc.
Definition: gr55xx_ll_pkc.h:298
ll_pkc_get_r1x_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r1x_pointer(pkc_regs_t *PKCx)
Get PKC parameter R1x pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:789
ll_pkc_get_tmp5_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmp5_pointer(pkc_regs_t *PKCx)
Get PKC parameter Tmp5 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1006
ll_pkc_get_x2_pointer
__STATIC_INLINE uint32_t ll_pkc_get_x2_pointer(pkc_regs_t *PKCx)
Get PKC parameter X2 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1130
ll_pkc_get_mi_v_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mi_v_pointer(pkc_regs_t *PKCx)
Get modular invertion parameter V pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1777
ll_pkc_struct_init
void ll_pkc_struct_init(ll_pkc_init_t *p_pkc_init)
Set each field of a ll_pkc_init_t type structure to default value.
ll_pkc_disable_software_start
__STATIC_INLINE void ll_pkc_disable_software_start(pkc_regs_t *PKCx)
Disable pkc start in software mode.
Definition: gr55xx_ll_pkc.h:1315
ll_pkc_disable_it_err
__STATIC_INLINE void ll_pkc_disable_it_err(pkc_regs_t *PKCx)
Disable the operation error interrupt.
Definition: gr55xx_ll_pkc.h:2245
ll_pkc_set_r0z_pointer
__STATIC_INLINE void ll_pkc_set_r0z_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R0z pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:743
ll_pkc_get_k_pointer
__STATIC_INLINE uint32_t ll_pkc_get_k_pointer(pkc_regs_t *PKCx)
Get PKC parameter k pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:479
ll_pkc_enable_it_done
__STATIC_INLINE void ll_pkc_enable_it_done(pkc_regs_t *PKCx)
Enable the operation done interrupt.
Definition: gr55xx_ll_pkc.h:2185
ll_pkc_is_enable_it_err
__STATIC_INLINE uint32_t ll_pkc_is_enable_it_err(pkc_regs_t *PKCx)
Indicate whether the operation error interrupt is enable.
Definition: gr55xx_ll_pkc.h:2290
_ll_ecc_curve_init::G
ll_ecc_point_t G
Definition: gr55xx_ll_pkc.h:117
ll_pkc_is_enabled_random_clock_gating
__STATIC_INLINE uint32_t ll_pkc_is_enabled_random_clock_gating(pkc_regs_t *PKCx)
Indicate whether the Random Clock Gating in software mode is enabled.
Definition: gr55xx_ll_pkc.h:1467
ll_pkc_set_rsq_pointer
__STATIC_INLINE void ll_pkc_set_rsq_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R^2 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:557
ll_pkc_get_mi_u_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mi_u_pointer(pkc_regs_t *PKCx)
Get modular invertion parameter U pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1746
ll_pkc_set_tmp3_pointer
__STATIC_INLINE void ll_pkc_set_tmp3_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Tmp3 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:929
ll_pkc_set_mas_a_pointer
__STATIC_INLINE void ll_pkc_set_mas_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular add/sub parameter A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1607
_ll_ecc_point::Y
uint32_t Y[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:95
ll_pkc_get_r0x_pointer
__STATIC_INLINE uint32_t ll_pkc_get_r0x_pointer(pkc_regs_t *PKCx)
Get PKC parameter R0x pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:696
ll_pkc_get_mik_output
__STATIC_INLINE uint32_t ll_pkc_get_mik_output(pkc_regs_t *PKCx)
Get K output in invertion operation.
Definition: gr55xx_ll_pkc.h:1916
ll_pkc_set_r0y_pointer
__STATIC_INLINE void ll_pkc_set_r0y_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter R0y pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:712
ll_pkc_is_enable_it_done
__STATIC_INLINE uint32_t ll_pkc_is_enable_it_done(pkc_regs_t *PKCx)
Indicate whether the operation done interrupt is enable.
Definition: gr55xx_ll_pkc.h:2275
ll_pkc_get_constant1_pointer
__STATIC_INLINE uint32_t ll_pkc_get_constant1_pointer(pkc_regs_t *PKCx)
Get PKC parameter Constant1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1068
ll_pkc_get_ecc_a_pointer
__STATIC_INLINE uint32_t ll_pkc_get_ecc_a_pointer(pkc_regs_t *PKCx)
Get ECC parameter A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1223
ll_pkc_set_tmp6_pointer
__STATIC_INLINE void ll_pkc_set_tmp6_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Tmp6 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1022
ll_pkc_enable_hardware_start
__STATIC_INLINE void ll_pkc_enable_hardware_start(pkc_regs_t *PKCx)
Enable pkc start in hardware mode.
Definition: gr55xx_ll_pkc.h:328
ll_pkc_get_mm_p_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mm_p_pointer(pkc_regs_t *PKCx)
Get modular multiplication parameter P pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1560
ll_pkc_enable_reset
__STATIC_INLINE void ll_pkc_enable_reset(pkc_regs_t *PKCx)
Enable pkc reset.
Definition: gr55xx_ll_pkc.h:418
ll_pkc_is_enabled_software_start
__STATIC_INLINE uint32_t ll_pkc_is_enabled_software_start(pkc_regs_t *PKCx)
Indicate whether the pkc start in software mode is enabled.
Definition: gr55xx_ll_pkc.h:1330
ll_pkc_is_enabled_software
__STATIC_INLINE uint32_t ll_pkc_is_enabled_software(pkc_regs_t *PKCx)
Indicate whether the pkc software mode is enabled.
Definition: gr55xx_ll_pkc.h:403
ll_pkc_disable_dummy_multi
__STATIC_INLINE void ll_pkc_disable_dummy_multi(pkc_regs_t *PKCx)
Disable Dummy Multi in software mode.
Definition: gr55xx_ll_pkc.h:1407
ll_pkc_set_p_pointer
__STATIC_INLINE void ll_pkc_set_p_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter p pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:526
ll_pkc_set_gz_pointer
__STATIC_INLINE void ll_pkc_set_gz_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Gz pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:650
ll_pkc_is_action_flag_it_err
__STATIC_INLINE uint32_t ll_pkc_is_action_flag_it_err(pkc_regs_t *PKCx)
Indicate whether the operation error interrupt is pending.
Definition: gr55xx_ll_pkc.h:2341
ll_pkc_set_mas_b_pointer
__STATIC_INLINE void ll_pkc_set_mas_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular add/sub parameter B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1638
ll_pkc_disable_hardware_start
__STATIC_INLINE void ll_pkc_disable_hardware_start(pkc_regs_t *PKCx)
Disable pkc start in hardware mode.
Definition: gr55xx_ll_pkc.h:343
ll_pkc_set_ba_a_pointer
__STATIC_INLINE void ll_pkc_set_ba_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set big integer operand A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2056
ll_pkc_get_tmp3_pointer
__STATIC_INLINE uint32_t ll_pkc_get_tmp3_pointer(pkc_regs_t *PKCx)
Get PKC parameter Tmp3 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:944
_ll_ecc_curve_init::B
uint32_t B[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:105
_ll_ecc_point::X
uint32_t X[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:93
ll_pkc_enable_random_clock_gating
__STATIC_INLINE void ll_pkc_enable_random_clock_gating(pkc_regs_t *PKCx)
Enable Random Clock Gating in software mode.
Definition: gr55xx_ll_pkc.h:1437
_ll_ecc_curve_init::N
uint32_t N[ECC_U32_LENGTH]
Definition: gr55xx_ll_pkc.h:111
ll_pkc_deinit
error_status_t ll_pkc_deinit(pkc_regs_t *PKCx)
De-initialize PKC registers (Registers restored to their default values).
ll_pkc_clear_flag_it_big_add_overflow
__STATIC_INLINE void ll_pkc_clear_flag_it_big_add_overflow(pkc_regs_t *PKCx)
Clear the big integer overflow interrupt flag.
Definition: gr55xx_ll_pkc.h:2401
ll_pkc_set_ba_b_pointer
__STATIC_INLINE void ll_pkc_set_ba_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set big integer operand B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2087
ll_pkc_get_mas_a_pointer
__STATIC_INLINE uint32_t ll_pkc_get_mas_a_pointer(pkc_regs_t *PKCx)
Get modular add/sub parameter A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1622
ll_pkc_enable_it_big_add_overflow
__STATIC_INLINE void ll_pkc_enable_it_big_add_overflow(pkc_regs_t *PKCx)
Enable the big integer overflow interrupt.
Definition: gr55xx_ll_pkc.h:2215
ll_pkc_set_constp
__STATIC_INLINE void ll_pkc_set_constp(pkc_regs_t *PKCx, uint32_t ConstP)
Set constant value for montgomery multiply in pkc sram.
Definition: gr55xx_ll_pkc.h:1270
ll_pkc_get_x1_pointer
__STATIC_INLINE uint32_t ll_pkc_get_x1_pointer(pkc_regs_t *PKCx)
Get PKC parameter X1 pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1099
ll_pkc_init_t
struct _ll_pkc_init ll_pkc_init_t
LL PKC Init Structure definition.
ll_pkc_set_gy_pointer
__STATIC_INLINE void ll_pkc_set_gy_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set PKC parameter Gy pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:619
ll_pkc_set_ecc_a_pointer
__STATIC_INLINE void ll_pkc_set_ecc_a_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set ECC parameter A pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1208
ll_ecc_point_t
struct _ll_ecc_point ll_ecc_point_t
LL PKC ECC Point Structure definition.
ll_pkc_get_dummy_multiply_seed
__STATIC_INLINE uint32_t ll_pkc_get_dummy_multiply_seed(pkc_regs_t *PKCx)
Get dummy multiply seed.
Definition: gr55xx_ll_pkc.h:1947
ll_pkc_enable_software
__STATIC_INLINE void ll_pkc_enable_software(pkc_regs_t *PKCx)
Enable pkc software mode.
Definition: gr55xx_ll_pkc.h:373
ll_pkc_set_bm_b_pointer
__STATIC_INLINE void ll_pkc_set_bm_b_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set big integer operand B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1994
ll_pkc_get_ba_b_pointer
__STATIC_INLINE uint32_t ll_pkc_get_ba_b_pointer(pkc_regs_t *PKCx)
Get big integer operand B pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:2102
ll_pkc_set_mi_u_pointer
__STATIC_INLINE void ll_pkc_set_mi_u_pointer(pkc_regs_t *PKCx, uint32_t pointer)
Set modular invertion parameter U pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1731
ll_pkc_get_swmi_tmp_pointer
__STATIC_INLINE uint32_t ll_pkc_get_swmi_tmp_pointer(pkc_regs_t *PKCx)
Get modular invertion parameter Tmp pointer in pkc sram.
Definition: gr55xx_ll_pkc.h:1870
ll_pkc_set_operation_mode
__STATIC_INLINE void ll_pkc_set_operation_mode(pkc_regs_t *PKCx, uint32_t operation_mode)
Set operation mode in software mode.
Definition: gr55xx_ll_pkc.h:1354
_ll_ecc_curve_init::ConstN
uint32_t ConstN
Definition: gr55xx_ll_pkc.h:113