Data Fields
ble_gattc_browse_srvc_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Client » Structures

GATTC Browse service(s) indication. More...

`#include <ble_gattc.h>`

## Data Fields
uint8_t | uuid_len
uint8_t | uuid [BLE_ATT_UUID_128_LEN]
uint16_t | start_hdl
uint16_t | end_hdl
union gattc_browse_attr_info | info [__ARRAY_EMPTY]

## Detailed Description

GATTC Browse service(s) indication.

## Field Documentation

## ◆ end_hdl

uint16_t ble_gattc_browse_srvc_t::end_hdl

Service end handle.

## ◆ info

union gattc_browse_attr_info ble_gattc_browse_srvc_t::info[__ARRAY_EMPTY]

Attribute information presented in the service(array length = end_hdl - start_hdl); If attr_type is equal to BLE_GATTC_BROWSE_NONE, the last attribute information has been found in previous one, although not reach the service end handle.

## ◆ start_hdl

uint16_t ble_gattc_browse_srvc_t::start_hdl

Service start handle.

## ◆ uuid

uint8_t ble_gattc_browse_srvc_t::uuid[BLE_ATT_UUID_128_LEN]

Service UUID.

## ◆ uuid_len

uint8_t ble_gattc_browse_srvc_t::uuid_len

Service UUID length.

The documentation for this struct was generated from the following file:

- ble_gattc.h