Macros
Alert Status BIT
BLE Services » Phone Alert Status Service (PASS) » Defines

PASS Alert Status bits. More...

## Macros
#define | PASS_NO_STATE_ACTIVE (0x00)
#define | PASS_RINGER_ACTIVE (0x01 << 0)
#define | PASS_VIBRATE_ACTIVE (0x01 << 1)
#define | PASS_DISPLAY_ALERT_ACTIVE (0x01 << 2)
#define | PASS_ALL_STATE_ACTIVE (0x07)

## Detailed Description

PASS Alert Status bits.

## Macro Definition Documentation

## ◆ PASS_ALL_STATE_ACTIVE

#define PASS_ALL_STATE_ACTIVE (0x07)

Bit for no state active.

## ◆ PASS_DISPLAY_ALERT_ACTIVE

#define PASS_DISPLAY_ALERT_ACTIVE (0x01 << 2)

Bit for display Alert Status State active.

## ◆ PASS_NO_STATE_ACTIVE

#define PASS_NO_STATE_ACTIVE (0x00)

Bit for no state active.

## ◆ PASS_RINGER_ACTIVE

#define PASS_RINGER_ACTIVE (0x01 << 0)

Bit for ringer State active.

## ◆ PASS_VIBRATE_ACTIVE

#define PASS_VIBRATE_ACTIVE (0x01 << 1)

Bit for vibrate State active.