Data Fields
ntf_source_pdu_t Struct Reference
BLE Services » Apple Notification Center Service (ANCS) » Structures

iOS notification structure. More...

`#include <ancs_protocol.h>`

## Data Fields
ancs_evt_id_t | event_id
ancs_ntf_flags_t | event_flags
ancs_category_id_t | category_id
uint8_t | category_count
uint32_t | notification_uid

## Detailed Description

iOS notification structure.

## Field Documentation

## ◆ category_count

uint8_t ntf_source_pdu_t::category_count

Current number of active notifications for this category ID.

## ◆ category_id

ancs_category_id_t ntf_source_pdu_t::category_id

Classification of the notification type, for example, email or location.

## ◆ event_flags

ancs_ntf_flags_t ntf_source_pdu_t::event_flags

Whether the notification was added, removed, or modified.

## ◆ event_id

ancs_evt_id_t ntf_source_pdu_t::event_id

Whether the notification was added, removed, or modified.

## ◆ notification_uid

uint32_t ntf_source_pdu_t::notification_uid

Notification UID.

The documentation for this struct was generated from the following file:

- ancs_protocol.h