Macros
Characteristic Properties
BLE » Attribute Protocol (ATT) » Defines

## Macros
#define | BLE_ATT_CHAR_PROP_BCAST 0x01
#define | BLE_ATT_CHAR_PROP_RD 0x02
#define | BLE_ATT_CHAR_PROP_WR_NO_RESP 0x04
#define | BLE_ATT_CHAR_PROP_WR 0x08
#define | BLE_ATT_CHAR_PROP_NTF 0x10
#define | BLE_ATT_CHAR_PROP_IND 0x20
#define | BLE_ATT_CHAR_PROP_AUTH 0x40
#define | BLE_ATT_CHAR_PROP_EXT_PROP 0x80

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_ATT_CHAR_PROP_AUTH

#define BLE_ATT_CHAR_PROP_AUTH 0x40

Characteristic Property: Authenticated Signed Writes.

## ◆ BLE_ATT_CHAR_PROP_BCAST

#define BLE_ATT_CHAR_PROP_BCAST 0x01

Characteristic Property: Broadcast.

## ◆ BLE_ATT_CHAR_PROP_EXT_PROP

#define BLE_ATT_CHAR_PROP_EXT_PROP 0x80

Characteristic Property: Extended Properties.

## ◆ BLE_ATT_CHAR_PROP_IND

#define BLE_ATT_CHAR_PROP_IND 0x20

Characteristic Property: Indicate.

## ◆ BLE_ATT_CHAR_PROP_NTF

#define BLE_ATT_CHAR_PROP_NTF 0x10

Characteristic Property: Notify.

## ◆ BLE_ATT_CHAR_PROP_RD

#define BLE_ATT_CHAR_PROP_RD 0x02

Characteristic Property: Read.

## ◆ BLE_ATT_CHAR_PROP_WR

#define BLE_ATT_CHAR_PROP_WR 0x08

Characteristic Property: Write.

## ◆ BLE_ATT_CHAR_PROP_WR_NO_RESP

#define BLE_ATT_CHAR_PROP_WR_NO_RESP 0x04

Characteristic Property: Write Without Response.