Data Fields
_calendar_alarm Struct Reference
Peripheral Driver » HAL Driver » CALENDAR » Structures » CALENDAR Time

CALENDAR_Alarm calendar alarm structure definition. More...

`#include <gr55xx_hal_calendar.h>`

## Data Fields
uint8_t | min
uint8_t | hour
uint8_t | alarm_sel
uint8_t | alarm_date_week_mask

## Detailed Description

CALENDAR_Alarm calendar alarm structure definition.

## Field Documentation

## ◆ alarm_date_week_mask

uint8_t _calendar_alarm::alarm_date_week_mask

Specifies the alarm date/weekday. If the alarm date is selected, this parameter must be set to a value in the 1 ~ 31 range. If the alarm weekday is selected, this parameter must be a value of CALENDAR Alarm weekday.

## ◆ alarm_sel

uint8_t _calendar_alarm::alarm_sel

Specifies the alarm is on date or weekday. This parameter can be a value of CALENDAR Alarm type select.

## ◆ hour

uint8_t _calendar_alarm::hour

Specifies the alarm time hour. This parameter must be a number between min_value = 0 and max_value = 23.

## ◆ min

uint8_t _calendar_alarm::min

Specifies the alarm time minutes. This parameter must be a number between min_value = 0 and max_value = 59.

The documentation for this struct was generated from the following file:

- gr55xx_hal_calendar.h