Data Fields
gap_init_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Legacy initiating parameters. More...

`#include <ble_gapm.h>`

## Data Fields
uint8_t | type
gap_bdaddr_t | peer_addr
uint16_t | interval_min
uint16_t | interval_max
uint16_t | slave_latency
uint16_t | sup_timeout
uint16_t | conn_timeout

## Detailed Description

Legacy initiating parameters.

## Field Documentation

## ◆ conn_timeout

uint16_t gap_init_param_t::conn_timeout

Timeout for connection establishment (in unit of 10ms). Cancel the procedure if connection has not been connected when the timeout occurs. 0 means there is no timeout.

## ◆ interval_max

uint16_t gap_init_param_t::interval_max

Maximum value for the connection interval (in unit of 1.25ms). Shall be greater than or equal to interval_min value. Allowed range is 7.5 ms to 4s.

## ◆ interval_min

uint16_t gap_init_param_t::interval_min

Minimum value for the connection interval (in unit of 1.25ms). Shall be less than or equal to interval_max value. Allowed range is 7.5 ms to 4s.

## ◆ peer_addr

gap_bdaddr_t gap_init_param_t::peer_addr

Peer device address.

## ◆ slave_latency

uint16_t gap_init_param_t::slave_latency

Slave latency. Number of events that can be missed by a connected slave device.

## ◆ sup_timeout

uint16_t gap_init_param_t::sup_timeout

Link supervision timeout (in unit of 10ms). Allowed range is 100 ms to 32s.

## ◆ type

uint8_t gap_init_param_t::type

Initiating type (see enum gap_init_type_t).

The documentation for this struct was generated from the following file:

- ble_gapm.h