Data Fields
_rng_init Struct Reference
Peripheral Driver » HAL Driver » RNG » Structures » RNG Configuration

RNG init structure definition. More...

`#include <gr55xx_hal_rng.h>`

## Data Fields
uint32_t | seed_mode
uint32_t | lfsr_mode
uint32_t | out_mode
uint32_t | post_mode

## Detailed Description

RNG init structure definition.

## Field Documentation

## ◆ lfsr_mode

uint32_t _rng_init::lfsr_mode

Specifies the configuration mode for the LFSR. This parameter can be a value of LFSR configuration mode

## ◆ out_mode

uint32_t _rng_init::out_mode

Specifies the Output mode for the RNG. This parameter can be a value of RNG Output mode

## ◆ post_mode

uint32_t _rng_init::post_mode

Specifies post-process configuration for the RNG. This parameter can be a value of Post-process mode

## ◆ seed_mode

uint32_t _rng_init::seed_mode

Specifies the seed source for the LFSR. This parameter can be a value of LFSR seed source

The documentation for this struct was generated from the following file:

- gr55xx_hal_rng.h