### - r -

- racp_filter_type : gls_racp_filter_t
- racp_operator : gls_racp_filter_t , gls_racp_rsp_t
- rand : sec_oob_t
- random_data : app_rng_evt_t
- random_func : pkc_init_t
- random_number : _rng_handle
- read : hci_uart_call_t
- read_cmd : _ll_xqspi_init_t , _xqspi_init_t
- read_fifo : _i2s_handle , _qspi_handle , _spi_handle
- read_rsp : dis_c_evt_t
- read_write_fifo : _spi_handle
- reason : lecb_disconn_ind_t
- received_length : ags_stream_env_t
- ref : hids_report_int_t
- ref_source : _ll_adc_init , _ll_comp_init
- ref_time_info : cts_adj_info_t , cts_c_evt_t , cts_init_t
- ref_value : _ll_adc_init , _ll_comp_init
- reg_cert_data_list : dis_init_t
- regi_user_name_present : uds_regi_user_data_flag_t
- remain_connectable : ble_escs_init_params_t
- REMAP : FPB_REG_TypeDef
- report_id : hids_report_ref_t
- report_map : hids_init_t
- report_type : hids_evt_t , hids_report_ref_t
- req_type : sec_cfm_enc_t , sec_enc_req_t
- reserved : ags_header_first_ext_t , ags_header_first_t , boot_info_t , uds_regi_user_data_flag_t
- reserved_1 : ags_ack_packet_t
- reserved_2 : ags_ack_packet_t
- reset_mode : _wdt_init
- result_code : ags_ack_packet_t
- retention : _adc_handle , _aes_handle , _comp_handle , _dma_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pkc_handle , _qspi_handle , _rng_handle , _spi_handle , _uart_handle , pwm_handle_t
- retry : _exflash_handle , _xqspi_handle_t
- right_rate : thscps_test_info_t
- ringer_set : pass_c_evt_t
- ringer_setting : pass_init_t
- rkey_dist : sec_param_t
- rng_msp_deinit : _hal_rng_callback
- rng_msp_init : _hal_rng_callback
- rng_ready_data_callback : _hal_rng_callback
- role : app_i2c_params_t
- rr_intervals : hrs_c_hr_meas_t
- rr_intervals_num : hrs_c_hr_meas_t
- rsc_feature : rscs_c_evt_t
- rsc_meas_buff : rscs_c_evt_t
- rsc_sensor_loc : rscs_c_evt_t
- rscs_ctrl_pt_cccd_handle : rscs_c_handles_t
- rscs_ctrl_pt_handle : rscs_c_handles_t
- rscs_rsc_feature_handle : rscs_c_handles_t
- rscs_rsc_meas_cccd_handle : rscs_c_handles_t
- rscs_rsc_meas_handle : rscs_c_handles_t
- rscs_sensor_loc_handle : rscs_c_handles_t
- rscs_srvc_end_handle : rscs_c_handles_t
- rscs_srvc_start_handle : rscs_c_handles_t
- rsp : gls_racp_rsp_t
- rsp_id : hrrcps_rsp_val_t
- rsp_param : hrrcps_rsp_val_t
- rssi : gap_conn_info_t , gap_ext_adv_report_ind_t , thscps_test_info_t
- rssi_cali : rf_trim_info_t
- rsvd : gap_ext_scan_param_t , gap_per_sync_param_t
- rts : app_uart_pin_cfg_t
- run_addr : boot_info_t
- rx : app_uart_pin_cfg_t
- rx_crc_err_cnt : link_rx_info_t
- rx_dma_channel : app_i2c_mode_t , app_i2s_mode_t , app_spi_mode_t , app_uart_mode_t
- rx_handler_cb : gdx_lcp_config_t
- rx_mic_err_cnt : link_rx_info_t
- rx_normal_cnt : link_rx_info_t
- rx_other_err_cnt : link_rx_info_t
- rx_path_comp : gap_dev_rf_path_comp_ind_t
- rx_phy : gap_le_phy_ind_t , thscps_test_conn_info_t
- rx_sample_delay : _ll_qspi_init_t , _qspi_init_t
- rx_sn_err_cnt : link_rx_info_t
- rx_state : _iso7816_handle_t , _uart_handle
- rx_sync_err_cnt : link_rx_info_t
- rx_threshold : _ll_i2s_init_t
- rx_timeout_mode : _uart_init
- rx_total_cnt : link_rx_info_t
- rx_xfer_count : _i2s_handle , _iso7816_handle_t , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- rx_xfer_size : _i2s_handle , _iso7816_handle_t , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- rxdata_size : _ll_i2s_init_t