Macros
Defines
BLE Services » Log Notification Service (LNS)

## Macros
#define | LNS_CONNECTION_MAX
#define | LNS_SERVICE_UUID
#define | LNS_LOG_INFO_VAL_LEN 244
#define | LNS_LOG_CTRL_PT_VAL_LEN 1

## Detailed Description

## Macro Definition Documentation

## ◆ LNS_CONNECTION_MAX

#define LNS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Log Notification Service connections.

## ◆ LNS_LOG_CTRL_PT_VAL_LEN

#define LNS_LOG_CTRL_PT_VAL_LEN 1

Length of Log Control Point value.

## ◆ LNS_LOG_INFO_VAL_LEN

#define LNS_LOG_INFO_VAL_LEN 244

Length of Log Information value.

## ◆ LNS_SERVICE_UUID

#define LNS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x08, 0xED, 0xA6

The UUID of Log Notification Service for setting advertising data.