Data Fields
gls_racp_rsp_t Struct Reference
BLE Services » Glucose Service Record Access Control Point (GLS_RACP) » Structures

Glucose Recoerd Access Control Point response value. More...

`#include <gls_racp.h>`

## Data Fields
gls_racp_op_code_t | op_code
gls_racp_operator_t | racp_operator
union {
uint16_t num_of_record
struct {
gls_racp_op_code_t op_code_req
gls_racp_operand_t status
} rsp
} | operand

## Detailed Description

Glucose Recoerd Access Control Point response value.

## Field Documentation

## ◆ num_of_record

uint16_t gls_racp_rsp_t::num_of_record

Number of record (if op_code = GLS_RACP_OP_REP_NB_OF_STRD_RECS).

## ◆ op_code

gls_racp_op_code_t gls_racp_rsp_t::op_code

Glucose Recoerd Access Control Point Operation Code.

## ◆ op_code_req

gls_racp_op_code_t gls_racp_rsp_t::op_code_req

Request Op Code.

## ◆ operand

union { ... } gls_racp_rsp_t::operand

Response operand.

## ◆ racp_operator

gls_racp_operator_t gls_racp_rsp_t::racp_operator

Glucose Recoerd Access Control Point Operator.

## ◆ rsp

struct { ... } gls_racp_rsp_t::rsp

Response.

## ◆ status

gls_racp_operand_t gls_racp_rsp_t::status

Command Status (if op_code = GLS_RACP_OP_RSP_CODE).

The documentation for this struct was generated from the following file:

- gls_racp.h