Data Fields
cts_adj_info_t Struct Reference
BLE Services » Current Time Service (CTS) » Structures

CTS Adjust information. More...

`#include <cts.h>`

## Data Fields
uint8_t | adjust_reason
cts_exact_time_256_t | day_date_time
cts_loc_time_info_t | loc_time_info
cts_ref_time_info_t | ref_time_info

## Detailed Description

CTS Adjust information.

## Field Documentation

## ◆ adjust_reason

uint8_t cts_adj_info_t::adjust_reason

Adjust Reason.

## ◆ day_date_time

cts_exact_time_256_t cts_adj_info_t::day_date_time

Exact Time 256.

## ◆ loc_time_info

cts_loc_time_info_t cts_adj_info_t::loc_time_info

Local Time information.

## ◆ ref_time_info

cts_ref_time_info_t cts_adj_info_t::ref_time_info

Reference Time information.

The documentation for this struct was generated from the following file:

- cts.h