Data Fields
gap_dev_tx_power_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

TX power info struct. More...

`#include <ble_gapc.h>`

## Data Fields
int8_t | min_tx_pwr
int8_t | max_tx_pwr

## Detailed Description

TX power info struct.

## Field Documentation

## ◆ max_tx_pwr

int8_t gap_dev_tx_power_t::max_tx_pwr

MAX of TX power. Size: 1 octet (signed integer). Range: -127 to +126. Unit: dBm.

## ◆ min_tx_pwr

int8_t gap_dev_tx_power_t::min_tx_pwr

MIN of TX power. Size: 1 octet (signed integer). Range: -127 to +126. Unit: dBm.

The documentation for this struct was generated from the following file:

- ble_gapc.h