Data Fields
uds_evt_t Struct Reference
BLE Services » User Data Service (UDS) » Structures

User Data Service event. More...

`#include <uds.h>`

## Data Fields
uint8_t | conn_idx
uds_evt_type_t | evt_type
const uint8_t * | p_data
uint16_t | length
uint16_t | consent_code
uds_chars_val_t | uds_chars_val
uint32_t | db_change_incr_val

## Detailed Description

User Data Service event.

## Field Documentation

## ◆ conn_idx

uint8_t uds_evt_t::conn_idx

The index of the connection.

## ◆ consent_code

uint16_t uds_evt_t::consent_code

Consent Code data.

## ◆ db_change_incr_val

uint32_t uds_evt_t::db_change_incr_val

Database Change Increment value set by peer.

## ◆ evt_type

uds_evt_type_t uds_evt_t::evt_type

The UDS event type.

## ◆ length

uint16_t uds_evt_t::length

Length of event data.

## ◆ p_data

const uint8_t* uds_evt_t::p_data

Pointer to event data.

## ◆ uds_chars_val

uds_chars_val_t uds_evt_t::uds_chars_val

UDS Characteristics value set by peer.

The documentation for this struct was generated from the following file:

- uds.h