Macros
CTS Pin State
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants

## Macros
#define | LL_UART_CTSPIN_STATE_ACTIVE 0x00000001U
#define | LL_UART_CTSPIN_STATE_INACTIVE 0x00000000U

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_CTSPIN_STATE_ACTIVE

#define LL_UART_CTSPIN_STATE_ACTIVE 0x00000001U

CTS pin active(Logic 1)

## ◆ LL_UART_CTSPIN_STATE_INACTIVE

#define LL_UART_CTSPIN_STATE_INACTIVE 0x00000000U

CTS pin pin inactive(Logic 0)