Macros
Post-process mode
Peripheral Driver » LL Driver » RNG » Defines » RNG Exported Constants

## Macros
#define | LL_RNG_POST_PRO_NOT (0x00000000UL)
#define | LL_RNG_POST_PRO_SKIPPING (1UL << RNG_CONFIG_POST_MODE_Pos)
#define | LL_RNG_POST_PRO_COUNTING (2UL << RNG_CONFIG_POST_MODE_Pos)
#define | LL_RNG_POST_PRO_NEUMANN (3UL << RNG_CONFIG_POST_MODE_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_RNG_POST_PRO_COUNTING

#define LL_RNG_POST_PRO_COUNTING (2UL << RNG_CONFIG_POST_MODE_Pos)

bit counting.

## ◆ LL_RNG_POST_PRO_NEUMANN

#define LL_RNG_POST_PRO_NEUMANN (3UL << RNG_CONFIG_POST_MODE_Pos)

Von-Neumann.

## ◆ LL_RNG_POST_PRO_NOT

#define LL_RNG_POST_PRO_NOT (0x00000000UL)

No post process.

## ◆ LL_RNG_POST_PRO_SKIPPING

#define LL_RNG_POST_PRO_SKIPPING (1UL << RNG_CONFIG_POST_MODE_Pos)

bit skipping.