### - a -

- A : _ll_ecc_curve_init
- accept : lecb_cfm_conn_t , sec_cfm_enc_t
- access_address : gdx_lcp_config_t
- accuracy : cts_c_ref_time_info_t , cts_ref_time_info_t
- ack_flag : ags_header_base_t , ags_stream_env_t
- action_set : thscps_evt_t
- active_channel : app_pwm_params_t , pwm_handle_t
- active_slot_no : ble_escs_init_params_t
- adc_conv_cplt_callback : _adc_callback
- adc_msp_deinit : _adc_callback
- adc_msp_init : _adc_callback
- adc_temp : adc_trim_info_t
- addr : _xqspi_command_t , gap_addr_t
- addr_size : _xqspi_command_t
- addr_type : gap_bdaddr_t , gap_peer_name_ind_t
- address : _qspi_command_t
- address_size : _ll_qspi_init_t , _qspi_command_t
- addressing_mode : _i2c_init
- adjust_reason : cts_adj_info_t , cts_c_cur_time_t , cts_cur_time_t
- adv_addr : gap_per_sync_param_t
- adv_info : gap_ext_adv_report_ind_t
- adv_interval : ble_escs_init_params_t
- adv_intv_max : gap_adv_param_t , gap_adv_period_cfg_t , gap_adv_prim_cfg_t
- adv_intv_min : gap_adv_param_t , gap_adv_period_cfg_t , gap_adv_prim_cfg_t
- adv_mode : gap_adv_param_t
- adv_name : dfu_adv_name_info_t
- adv_name_length : dfu_adv_name_info_t
- adv_param : thscps_evt_t
- adv_sid : gap_adv_second_cfg_t , gap_ext_adv_report_ind_t , gap_period_adv_addr_cfg_t , gap_sync_established_ind_t
- adv_tx_power : ble_escs_init_params_t , gap_dev_info_t
- adv_type : gap_ext_adv_report_ind_t
- aes_abort_cplt_callback : _aes_callback
- aes_done_callback : _aes_callback
- aes_error_callback : _aes_callback
- aes_mask : _keyram_mask
- aes_msp_deinit : _aes_callback
- aes_msp_init : _aes_callback
- age : uds_chars_val_t
- age_present : uds_chars_flag_t
- ags_alexa_stream_cb : ags_init_t
- ags_control_stream_cb : ags_init_t
- alarm : _calendar_handle
- alarm_counter : _aon_wdt_init
- alarm_date_week_mask : _calendar_alarm
- alarm_sel : _calendar_alarm
- alert_level : ias_evt_t , lls_c_evt_t , lls_evt_t
- alert_num : ans_c_new_alert_t , ans_new_alert_t
- alert_status : pass_c_evt_t , pass_init_t
- align : _ll_pwm_init_t , pwm_init_t
- ams_attr_display_handle : ams_c_handles_t
- ams_attr_update_cccd_handle : ams_c_handles_t
- ams_attr_update_handle : ams_c_handles_t
- ams_cmd_cccd_handle : ams_c_handles_t
- ams_cmd_handle : ams_c_handles_t
- ams_srvc_end_handle : ams_c_handles_t
- ams_srvc_start_handle : ams_c_handles_t
- ancs_control_point_handle : ancs_c_att_handles_t
- ancs_data_source_cccd_handle : ancs_c_att_handles_t
- ancs_data_source_handle : ancs_c_att_handles_t
- ancs_ntf_source_cccd_handle : ancs_c_att_handles_t
- ancs_ntf_source_handle : ancs_c_att_handles_t
- ancs_service_handle : ancs_c_att_handles_t
- ans_ctrl_pt_handle : ans_c_handles_t
- ans_new_alert_cccd_handle : ans_c_handles_t
- ans_new_alert_handle : ans_c_handles_t
- ans_srvc_end_handle : ans_c_handles_t
- ans_srvc_start_handle : ans_c_handles_t
- ans_sup_new_alert_cat_handle : ans_c_handles_t
- ans_sup_unread_alert_cat_handle : ans_c_handles_t
- ans_unread_alert_cccd_handle : ans_c_handles_t
- ans_unread_alert_handle : ans_c_handles_t
- aon_gpio_callback : _aon_gpio_callback
- aon_wdt_alarm_callback : _aon_wdt_callback
- app_ble_init_cmp_callback : app_callback_t
- app_gap_adv_data_update_cb : gap_cb_fun_t
- app_gap_adv_report_ind_cb : gap_cb_fun_t
- app_gap_adv_start_cb : gap_cb_fun_t
- app_gap_adv_stop_cb : gap_cb_fun_t
- app_gap_auto_connection_timeout_cb : gap_cb_fun_t
- app_gap_callbacks : app_callback_t
- app_gap_connect_cancel_cb : gap_cb_fun_t
- app_gap_connect_cb : gap_cb_fun_t
- app_gap_connection_info_get_cb : gap_cb_fun_t
- app_gap_connection_update_cb : gap_cb_fun_t
- app_gap_connection_update_req_cb : gap_cb_fun_t
- app_gap_dev_info_get_cb : gap_cb_fun_t
- app_gap_disconnect_cb : gap_cb_fun_t
- app_gap_le_pkt_size_info_cb : gap_cb_fun_t
- app_gap_param_set_cb : gap_cb_fun_t
- app_gap_peer_info_get_cb : gap_cb_fun_t
- app_gap_peer_name_ind_cb : gap_cb_fun_t
- app_gap_phy_update_cb : gap_cb_fun_t
- app_gap_psm_manager_cb : gap_cb_fun_t
- app_gap_rslv_addr_read_cb : gap_cb_fun_t
- app_gap_scan_req_ind_cb : gap_cb_fun_t
- app_gap_scan_start_cb : gap_cb_fun_t
- app_gap_scan_stop_cb : gap_cb_fun_t
- app_gap_stop_sync_cb : gap_cb_fun_t
- app_gap_sync_establish_cb : gap_cb_fun_t
- app_gap_sync_lost_cb : gap_cb_fun_t
- app_gatt_common_callback : app_callback_t
- app_gatt_mtu_exchange_cb : gatt_common_cb_fun_t
- app_gatt_prf_register_cb : gatt_common_cb_fun_t
- app_gattc_callback : app_callback_t
- app_gattc_char_desc_disc_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_char_disc_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_inc_srvc_disc_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_ntf_ind_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_prf_reg_cb : gattc_prf_cbs_t
- app_gattc_read_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_srvc_browse_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_srvc_disc_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gattc_write_cb : gattc_cb_fun_t , gattc_prf_cbs_t
- app_gatts_cccd_set_cb : gatts_prf_cbs_t
- app_gatts_ntf_ind_cb : gatts_prf_cbs_t
- app_gatts_prep_write_cb : gatts_prf_cbs_t
- app_gatts_read_cb : gatts_prf_cbs_t
- app_gatts_write_cb : gatts_prf_cbs_t
- app_l2cap_lecb_add_credits_ind_cb : l2cap_lecb_cb_fun_t
- app_l2cap_lecb_conn_cb : l2cap_lecb_cb_fun_t
- app_l2cap_lecb_conn_req_cb : l2cap_lecb_cb_fun_t
- app_l2cap_lecb_credit_add_cmp_cb : l2cap_lecb_cb_fun_t
- app_l2cap_lecb_disconn_cb : l2cap_lecb_cb_fun_t
- app_l2cap_lecb_sdu_recv_cb : l2cap_lecb_cb_fun_t
- app_l2cap_lecb_sdu_send_cb : l2cap_lecb_cb_fun_t
- app_prepare_for_sleep : app_sleep_callbacks_t
- app_sec_callback : app_callback_t
- app_sec_enc_ind_cb : sec_cb_fun_t
- app_sec_enc_req_cb : sec_cb_fun_t
- app_sec_key_missing_cb : sec_cb_fun_t
- app_sec_keypress_notify_cb : sec_cb_fun_t
- app_sleep_canceled : app_sleep_callbacks_t
- app_wake_up_ind : app_sleep_callbacks_t
- assert_err_cb : sys_assert_cb_t
- assert_param_cb : sys_assert_cb_t
- assert_warn_cb : sys_assert_cb_t
- attr : gattc_browse_attr_info
- attr_char : gattc_browse_attr_info
- attr_count : ams_c_ett_attr_id_t
- attr_hdl : ble_gattc_desc_t , ble_gattc_include_t
- attr_id : ams_c_attr_info_t , ams_c_ett_attr_id_t
- attr_info : ams_c_evt_t
- attr_tab : gatts_create_db_t
- attr_tab_128 : gatts_create_db_t::attribute_table
- attr_tab_16 : gatts_create_db_t::attribute_table
- attr_tab_cfg : gatts_create_db_t
- attr_tab_type : gatts_create_db_t
- attr_type : gattc_browse_attr_char_t , gattc_browse_attr_info , gattc_browse_attr_t , gattc_browse_inc_srvc_t
- audio_freq : _i2s_init , _ll_i2s_init_t
- auth : sec_param_t
- auto_reload : _dual_timer_init , _ll_dual_timer_init , _ll_timer_init_t , _timer_init
- average_val : thscps_test_info_t