Data Fields
pass_c_evt_t Struct Reference
BLE Services » Phone Alert Status Service Client (PASS_C) » Structures

Phone Alert Status Client Service event. More...

`#include <pass_c.h>`

## Data Fields
uint8_t | conn_idx
pass_c_evt_type_t | evt_type
union {
uint8_t alert_status
uint8_t ringer_set
} | value

## Detailed Description

Phone Alert Status Client Service event.

## Field Documentation

## ◆ alert_status

uint8_t pass_c_evt_t::alert_status

Alert status received.

## ◆ conn_idx

uint8_t pass_c_evt_t::conn_idx

The index of the connection.

## ◆ evt_type

pass_c_evt_type_t pass_c_evt_t::evt_type

The PASS event type.

## ◆ ringer_set

uint8_t pass_c_evt_t::ringer_set

Ringer setting received.

## ◆ value

union { ... } pass_c_evt_t::value

Value received.

The documentation for this struct was generated from the following file:

- pass_c.h