Data Fields
gap_dev_version_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

The struct of device version. More...

`#include <ble_gapc.h>`

## Data Fields
uint8_t | hci_ver
uint8_t | lmp_ver
uint8_t | host_ver
uint16_t | hci_subver
uint16_t | lmp_subver
uint16_t | host_subver
uint16_t | manuf_name

## Detailed Description

The struct of device version.

## Field Documentation

## ◆ hci_subver

uint16_t gap_dev_version_ind_t::hci_subver

HCI subversion.

## ◆ hci_ver

uint8_t gap_dev_version_ind_t::hci_ver

HCI version.

## ◆ host_subver

uint16_t gap_dev_version_ind_t::host_subver

Host subversion.

## ◆ host_ver

uint8_t gap_dev_version_ind_t::host_ver

Host version.

## ◆ lmp_subver

uint16_t gap_dev_version_ind_t::lmp_subver

LMP subversion.

## ◆ lmp_ver

uint8_t gap_dev_version_ind_t::lmp_ver

LMP version.

## ◆ manuf_name

uint16_t gap_dev_version_ind_t::manuf_name

Manufacturer name.

The documentation for this struct was generated from the following file:

- ble_gapc.h