Data Fields
bcs_init_t Struct Reference
BLE Services » Body Composition Service (BCS) » Structures

Body Composition Service Init variable. More...

`#include <bcs.h>`

## Data Fields
bcs_evt_handler_t | evt_handler
uint32_t | feature
uint8_t | char_mask
bcs_unit_t | bcs_unit
bcs_meas_flag_t | bcs_meas_flags
bcs_mass_res_t | bcs_mass_res
bcs_height_res_t | bcs_height_res

## Detailed Description

Body Composition Service Init variable.

## Field Documentation

## ◆ bcs_height_res

bcs_height_res_t bcs_init_t::bcs_height_res

Initial resolution of height value.

## ◆ bcs_mass_res

bcs_mass_res_t bcs_init_t::bcs_mass_res

Initial resolution of mass value.

## ◆ bcs_meas_flags

bcs_meas_flag_t bcs_init_t::bcs_meas_flags

Initial measurement flags.

## ◆ bcs_unit

bcs_unit_t bcs_init_t::bcs_unit

Initial unit system as SI or Imperial.

## ◆ char_mask

uint8_t bcs_init_t::char_mask

Initial mask of Supported characteristics, and configured with Characteristics Mask

## ◆ evt_handler

bcs_evt_handler_t bcs_init_t::evt_handler

Body Composition Service event handler.

## ◆ feature

uint32_t bcs_init_t::feature

Initial value for features.

The documentation for this struct was generated from the following file:

- bcs.h