Functions
FLAG_Management
Peripheral Driver » LL Driver » WDT » Functions

## Functions
__STATIC_INLINE uint32_t | ll_wdt_is_active_flag_it (wdt_regs_t *WDTx)
| Indicate if the WDT Interrupt Flag is set or not. More...
__STATIC_INLINE void | ll_wdt_clear_flag_it (wdt_regs_t *WDTx)
| Clear Interrupt Status flag. More...

## Detailed Description

## Function Documentation

## ◆ ll_wdt_clear_flag_it()

__STATIC_INLINE void ll_wdt_clear_flag_it | ( | wdt_regs_t * | WDTx | ) |

Clear Interrupt Status flag.

Register | BitsName
--- | ---
INTCLR | INTCLR

Parameters

  WDTx | WDT instance.

Return values

  None |

## ◆ ll_wdt_is_active_flag_it()

__STATIC_INLINE uint32_t ll_wdt_is_active_flag_it | ( | wdt_regs_t * | WDTx | ) |

Indicate if the WDT Interrupt Flag is set or not.

Note
  This bit is set by hardware when the counter has reached 0. It can be cleared by software by writing any value to the INTCLR Register.

Register | BitsName
--- | ---
MIS | INTSTAT

Parameters

  WDTx | WDT instance.

Return values

  State | of bit (1 or 0).