Data Fields
gap_conn_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

The parameter of connection. More...

`#include <ble_gapc.h>`

## Data Fields
uint16_t | interval_min
uint16_t | interval_max
uint16_t | slave_latency
uint16_t | sup_timeout

## Detailed Description

The parameter of connection.

## Field Documentation

## ◆ interval_max

uint16_t gap_conn_param_t::interval_max

Maximum value for the connection interval. This shall be greater than or equal to Conn_Interval_Min. Range: 0x0006 to 0x0C80, unit: 1.25 ms, time range: 7.5 ms to 4 s.

## ◆ interval_min

uint16_t gap_conn_param_t::interval_min

Minimum value for the connection interval. This shall be less than or equal to Conn_Interval_Max. Range: 0x0006 to 0x0C80, unit: 1.25 ms, time range: 7.5 ms to 4 s

## ◆ slave_latency

uint16_t gap_conn_param_t::slave_latency

Slave latency for the connection in number of connection events. Range: 0x0000 to 0x01F3.

## ◆ sup_timeout

uint16_t gap_conn_param_t::sup_timeout

Supervision timeout for the LE link. Range: 0x000A to 0x0C80, unit: 10 ms, time range: 100 ms to 32 s.

The documentation for this struct was generated from the following file:

- ble_gapc.h