Data Fields
cts_c_evt_t Struct Reference
BLE Services » Current Time Service Client (CTS_C) » Structures

Current Time Service Client event. More...

`#include <cts_c.h>`

## Data Fields
uint8_t | conn_idx
cts_c_evt_type_t | evt_type
union {
cts_c_cur_time_t cur_time
cts_c_loc_time_info_t loc_time_info
cts_c_ref_time_info_t ref_time_info
} | value

## Detailed Description

Current Time Service Client event.

## Field Documentation

## ◆ conn_idx

uint8_t cts_c_evt_t::conn_idx

The index of the connection.

## ◆ cur_time

cts_c_cur_time_t cts_c_evt_t::cur_time

Curren time received.

## ◆ evt_type

cts_c_evt_type_t cts_c_evt_t::evt_type

The CTS client event type.

## ◆ loc_time_info

cts_c_loc_time_info_t cts_c_evt_t::loc_time_info

Local time information received.

## ◆ ref_time_info

cts_c_ref_time_info_t cts_c_evt_t::ref_time_info

Referen time information received.

## ◆ value

union { ... } cts_c_evt_t::value

Decoded result of value received.

The documentation for this struct was generated from the following file:

- cts_c.h