Data Fields
gattc_write_no_resp_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Client » Structures

GATTC write without response structure. More...

`#include <ble_gattc.h>`

## Data Fields
bool | signed_write
uint16_t | handle
uint16_t | length
uint8_t * | p_value

## Detailed Description

GATTC write without response structure.

## Field Documentation

## ◆ handle

uint16_t gattc_write_no_resp_t::handle

Attribute handle.

## ◆ length

uint16_t gattc_write_no_resp_t::length

Write length.

## ◆ p_value

uint8_t* gattc_write_no_resp_t::p_value

Value to write.

## ◆ signed_write

bool gattc_write_no_resp_t::signed_write

True if signed write should be used when possible/applicable.

The documentation for this struct was generated from the following file:

- ble_gattc.h