Macros
XQSPI FIFO Threshold, FIFO depth is 64*4bytes, only in QSPI mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | XQSPI_FIFO_THRESHOLD_1_8 LL_XQSPI_QSPI_FIFO_WATERMARK_1_8
#define | XQSPI_FIFO_THRESHOLD_1_4 LL_XQSPI_QSPI_FIFO_WATERMARK_1_4
#define | XQSPI_FIFO_THRESHOLD_1_2 LL_XQSPI_QSPI_FIFO_WATERMARK_1_2
#define | XQSPI_FIFO_THRESHOLD_3_4 LL_XQSPI_QSPI_FIFO_WATERMARK_3_4
#define | XQSPI_FIFO_DEPTH LL_XQSPI_QSPI_FIFO_DEPTH

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_FIFO_DEPTH

#define XQSPI_FIFO_DEPTH LL_XQSPI_QSPI_FIFO_DEPTH

FIFO full depth

## ◆ XQSPI_FIFO_THRESHOLD_1_2

#define XQSPI_FIFO_THRESHOLD_1_2 LL_XQSPI_QSPI_FIFO_WATERMARK_1_2

FIFO depth/2

## ◆ XQSPI_FIFO_THRESHOLD_1_4

#define XQSPI_FIFO_THRESHOLD_1_4 LL_XQSPI_QSPI_FIFO_WATERMARK_1_4

FIFO depth/4

## ◆ XQSPI_FIFO_THRESHOLD_1_8

#define XQSPI_FIFO_THRESHOLD_1_8 LL_XQSPI_QSPI_FIFO_WATERMARK_1_8

FIFO depth/8

## ◆ XQSPI_FIFO_THRESHOLD_3_4

#define XQSPI_FIFO_THRESHOLD_3_4 LL_XQSPI_QSPI_FIFO_WATERMARK_3_4

FIFO depth*3/4