Macros
I2S Clock Source
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_CLOCK_SRC_96M (0x00000000UL)
#define | LL_I2S_CLOCK_SRC_32M (1UL << 18)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_CLOCK_SRC_32M

#define LL_I2S_CLOCK_SRC_32M (1UL << 18)

I2S clock source select: 32M

## ◆ LL_I2S_CLOCK_SRC_96M

#define LL_I2S_CLOCK_SRC_96M (0x00000000UL)

I2S clock source select: 96M