Data Fields
gus_c_evt_t Struct Reference
BLE Services » Goodix UART Service Client (GUS_C) » Structures

Goodix UART Service Client event. More...

`#include <gus_c.h>`

## Data Fields
uint8_t | conn_idx
gus_c_evt_type_t | evt_type
uint16_t | length
uint8_t * | p_data

## Detailed Description

Goodix UART Service Client event.

## Field Documentation

## ◆ conn_idx

uint8_t gus_c_evt_t::conn_idx

Connection index.

## ◆ evt_type

gus_c_evt_type_t gus_c_evt_t::evt_type

GUS Client event type.

## ◆ length

uint16_t gus_c_evt_t::length

Length of event data.

## ◆ p_data

uint8_t * gus_c_evt_t::p_data

Pointer to event data.

The documentation for this struct was generated from the following files:

- gus_c.h
- mlmr_c.h