Enumerations
Enumerations
BLE Services » Goodix UART Service (GUS)

## Enumerations
enum | gus_evt_type_t { GUS_EVT_INVALID, GUS_EVT_RX_DATA_RECEIVED, GUS_EVT_TX_DATA_SENT, GUS_EVT_TX_PORT_OPENED, GUS_EVT_TX_PORT_CLOSED, GUS_EVT_FLOW_CTRL_ENABLE, GUS_EVT_FLOW_CTRL_DISABLE, GUS_EVT_TX_FLOW_OFF, GUS_EVT_TX_FLOW_ON, GUS_EVT_INVALID, GUS_EVT_RX_DATA_RECEIVED, GUS_EVT_TX_DATA_SENT, GUS_EVT_TX_PORT_OPENED, GUS_EVT_TX_PORT_CLOSED, GUS_EVT_FLOW_CTRL_ENABLE, GUS_EVT_FLOW_CTRL_DISABLE, GUS_EVT_TX_FLOW_OFF, GUS_EVT_TX_FLOW_ON }
| Goodix UART Service event types. More...
enum | gus_evt_type_t { GUS_EVT_INVALID, GUS_EVT_RX_DATA_RECEIVED, GUS_EVT_TX_DATA_SENT, GUS_EVT_TX_PORT_OPENED, GUS_EVT_TX_PORT_CLOSED, GUS_EVT_FLOW_CTRL_ENABLE, GUS_EVT_FLOW_CTRL_DISABLE, GUS_EVT_TX_FLOW_OFF, GUS_EVT_TX_FLOW_ON, GUS_EVT_INVALID, GUS_EVT_RX_DATA_RECEIVED, GUS_EVT_TX_DATA_SENT, GUS_EVT_TX_PORT_OPENED, GUS_EVT_TX_PORT_CLOSED, GUS_EVT_FLOW_CTRL_ENABLE, GUS_EVT_FLOW_CTRL_DISABLE, GUS_EVT_TX_FLOW_OFF, GUS_EVT_TX_FLOW_ON }
| Goodix UART Service event types. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ gus_evt_type_t [1/2]

enum gus_evt_type_t

Goodix UART Service event types.

Enumerator
GUS_EVT_INVALID | Invalid GUS event.
GUS_EVT_RX_DATA_RECEIVED | The data from the peer has been received.
GUS_EVT_TX_DATA_SENT | The data from the application has been sent, and the service is ready to accept new data from the application.
GUS_EVT_TX_PORT_OPENED | Tx port has been opened.
GUS_EVT_TX_PORT_CLOSED | Tx port has been closed.
GUS_EVT_FLOW_CTRL_ENABLE | GUS flow control been enabled.
GUS_EVT_FLOW_CTRL_DISABLE | GUS flow control been disabled.
GUS_EVT_TX_FLOW_OFF | Tx flow off control request.
GUS_EVT_TX_FLOW_ON | Tx flow on control request.
GUS_EVT_INVALID | Invalid GUS event.
GUS_EVT_RX_DATA_RECEIVED | The data from the peer has been received.
GUS_EVT_TX_DATA_SENT | The data from the application has been sent, and the service is ready to accept new data from the application.
GUS_EVT_TX_PORT_OPENED | Tx port has been opened.
GUS_EVT_TX_PORT_CLOSED | Tx port has been closed.
GUS_EVT_FLOW_CTRL_ENABLE | GUS flow control been enabled.
GUS_EVT_FLOW_CTRL_DISABLE | GUS flow control been disabled.
GUS_EVT_TX_FLOW_OFF | Tx flow off control request.
GUS_EVT_TX_FLOW_ON | Tx flow on control request.

## ◆ gus_evt_type_t [2/2]

enum gus_evt_type_t

Goodix UART Service event types.

Enumerator
GUS_EVT_INVALID | Invalid GUS event.
GUS_EVT_RX_DATA_RECEIVED | The data from the peer has been received.
GUS_EVT_TX_DATA_SENT | The data from the application has been sent, and the service is ready to accept new data from the application.
GUS_EVT_TX_PORT_OPENED | Tx port has been opened.
GUS_EVT_TX_PORT_CLOSED | Tx port has been closed.
GUS_EVT_FLOW_CTRL_ENABLE | GUS flow control been enabled.
GUS_EVT_FLOW_CTRL_DISABLE | GUS flow control been disabled.
GUS_EVT_TX_FLOW_OFF | Tx flow off control request.
GUS_EVT_TX_FLOW_ON | Tx flow on control request.
GUS_EVT_INVALID | Invalid GUS event.
GUS_EVT_RX_DATA_RECEIVED | The data from the peer has been received.
GUS_EVT_TX_DATA_SENT | The data from the application has been sent, and the service is ready to accept new data from the application.
GUS_EVT_TX_PORT_OPENED | Tx port has been opened.
GUS_EVT_TX_PORT_CLOSED | Tx port has been closed.
GUS_EVT_FLOW_CTRL_ENABLE | GUS flow control been enabled.
GUS_EVT_FLOW_CTRL_DISABLE | GUS flow control been disabled.
GUS_EVT_TX_FLOW_OFF | Tx flow off control request.
GUS_EVT_TX_FLOW_ON | Tx flow on control request.