Data Structures | Typedefs
Structures
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control

## Data Structures
struct | gap_dev_version_ind_t
| The struct of device version. More...
struct | gap_addr_t
| The struct of address. More...
struct | gap_bdaddr_t
| The struct of broadcast address with broadcast type. More...
struct | gap_get_bd_addr_t
| Get broadcast address struct. More...
struct | gap_dev_adv_tx_power_t
| TX power info struct. More...
struct | gap_dev_tx_power_t
| TX power info struct. More...
struct | gap_max_data_len_t
| Max data length info struct. More...
struct | gap_sugg_dflt_data_len_t
| Suggested default data length info. More...
struct | gap_nb_adv_sets_t
| Number of available advertising sets info. More...
struct | gap_max_adv_data_len_ind_t
| Maximum advertising data length info. More...
struct | gap_dev_rf_path_comp_ind_t
| RF path compensation values info. More...
union | gap_dev_info_t
| Device info. More...
struct | gap_dev_info_get_t
| Get device info operation struct. More...
struct | gap_rslv_addr_read_t
| Read resolvable address info struct. More...
struct | gap_sync_established_ind_t
| Sync established indication. More...
struct | gap_ext_adv_report_ind_t
| APP receives the extended advertising report indication info struct. More...
struct | gap_peer_name_ind_t
| Name of peer device indication. More...
struct | gap_conn_update_cmp_t
| Connection parameter used to update connection parameters. More...
struct | gap_conn_param_t
| The parameter of connection. More...
struct | gap_conn_update_param_t
| The parameter of update connection. More...
struct | gap_conn_cmp_t
| Connection complete info. More...
struct | gap_chnl_map_t
| Channel map structure. More...
struct | gap_le_phy_ind_t
| PHY info. More...
union | gap_conn_info_t
| Connection info. More...
struct | gap_conn_info_param_t
| The info of connecting operation. More...
struct | gap_peer_version_ind_t
| Peer version info. More...
struct | gap_peer_features_ind_t
| LE features info. More...
union | gap_peer_info_t
| LE peer info. More...
struct | gap_peer_info_param_t
| Get peer info operation struct. More...
struct | gap_le_pkt_size_ind_t
| Supported data length size Indication. More...
struct | gap_con_plan_tag_t
| The Structure for BLE Connection Arrangement. More...
struct | gap_set_pref_slave_evt_dur_param_t
| Set preference slave event duration. More...
struct | gap_cb_fun_t
| The gap callback function struct. More...

## Typedefs
typedef void(* | app_ble_init_cmp_cb_t) (void)
| BLE initialization completed callback function for application.

## Detailed Description