Data Fields
ags_header_first_ext_t Struct Reference
BLE Services » Alexa Gadget Service (AGS) » Structures

Alexa Gadget Service extended version of header in first packet. More...

`#include <ags.h>`

## Data Fields
ags_header_base_t | header_base
uint8_t | reserved
uint8_t | total_trxn_length [2]
uint8_t | payload_length [2]

## Detailed Description

Alexa Gadget Service extended version of header in first packet.

## Field Documentation

## ◆ header_base

ags_header_base_t ags_header_first_ext_t::header_base

Header base.

## ◆ payload_length

uint8_t ags_header_first_ext_t::payload_length[2]

Payload Length.

## ◆ reserved

uint8_t ags_header_first_ext_t::reserved

Reserved. This is only present in the first packet of the transaction.

## ◆ total_trxn_length

uint8_t ags_header_first_ext_t::total_trxn_length[2]

Total transaction length. This is only present in the first packet of the transaction.

The documentation for this struct was generated from the following file:

- ags.h