Data Structures | Macros | Typedefs | Enumerations | Functions
hids.h File Reference

Human Interface Device Service API. More...

`#include "ble_prf_utils.h"`
`#include "gr55xx_sys.h"`
`#include "custom_config.h"`
`#include <stdint.h>`

Go to the source code of this file.

## Data Structures
struct | hids_evt_t
| HID Service event. More...
struct | hids_hid_info_t
| HID Information characteristic value. More...
struct | hids_report_ref_t
| Value of a Report Reference descriptor. More...
struct | hids_report_int_t
| HID Service Report characteristic define. More...
struct | hids_report_map_t
| HID Service Report Map characteristic value. More...
struct | hids_init_t
| HID Service initialization variable. More...

## Macros
#define | HIDS_CONNECTION_MAX
#define | HIDS_REPORT_MAX_SIZE 20
#define | HIDS_REPORT_MAP_MAX_SIZE 512
#define | HIDS_REP_TYPE_INPUT 1
#define | HIDS_REP_TYPE_OUTPUT 2
#define | HIDS_REP_TYPE_FEATURE 3
#define | HID_INFO_FLAG_REMOTE_WAKE_MSK 0x01
#define | HID_INFO_FLAG_NORMALLY_CONNECTABLE_MSK 0x02

## Typedefs
typedef void(* | hids_evt_handler_t) (hids_evt_t *p_evt)
| HID Service event handler type. More...

## Enumerations
enum | hids_evt_type_t { HIDS_EVT_INVALID, HIDS_EVT_IN_REP_NOTIFY_ENABLED, HIDS_EVT_IN_REP_NOTIFY_DISABLED, HIDS_EVT_HOST_SUSP, HIDS_EVT_HOST_EXIT_SUSP, HIDS_EVT_BOOT_MODE_ENTERED, HIDS_EVT_REPORT_MODE_ENTERED, HIDS_EVT_REP_CHAR_WRITE }
| HID Service event type. More...
enum | hids_report_type_t { HIDS_REPORT_TYPE_RESERVED, HIDS_REPORT_TYPE_IN1, HIDS_REPORT_TYPE_IN2, HIDS_REPORT_TYPE_IN3, HIDS_REPORT_TYPE_OUT, HIDS_REPORT_TYPE_FEATURE, HIDS_REPORT_TYPE_KB_IN, HIDS_REPORT_TYPE_KB_OUT, HIDS_REPORT_TYPE_MOUSE_IN }
| HID Service write report type. More...

## Functions
sdk_err_t | hids_service_init (hids_init_t *p_hids_init)
| Initialize a HID Service instance in ATT DB. More...
sdk_err_t | hids_input_rep_send (uint8_t conn_idx, uint8_t rep_idx, uint8_t *p_data, uint16_t length)
| Send an input report. More...
sdk_err_t | hids_boot_kb_in_rep_send (uint8_t conn_idx, uint8_t *p_data, uint16_t length)
| Send boot keyboard input report. More...
sdk_err_t | hids_boot_mouse_in_rep_send (uint8_t conn_idx, uint8_t *p_data, uint16_t length)
| Send boot mouse input report. More...

## Detailed Description

Human Interface Device Service API.

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.