Data Fields
gus_evt_t Struct Reference
BLE Services » Goodix UART Service (GUS) » Structures

Goodix UART Service event. More...

`#include <gus.h>`

## Data Fields
gus_evt_type_t | evt_type
uint8_t | conn_idx
uint8_t * | p_data
uint16_t | length

## Detailed Description

Goodix UART Service event.

## Field Documentation

## ◆ conn_idx

uint8_t gus_evt_t::conn_idx

The index of the connection for the data transmission.

## ◆ evt_type

gus_evt_type_t gus_evt_t::evt_type

The GUS event.

## ◆ length

uint16_t gus_evt_t::length

Length of received data.

## ◆ p_data

uint8_t * gus_evt_t::p_data

Pointer to the buffer within received data.

The documentation for this struct was generated from the following files:

- gus.h
- mlmr.h