Data Fields
cts_evt_t Struct Reference
BLE Services » Current Time Service (CTS) » Structures

Current Time Service event. More...

`#include <cts.h>`

## Data Fields
uint8_t | conn_idx
cts_evt_type_t | evt_type
const uint8_t * | p_data
uint16_t | length
cts_cur_time_t | cur_time
cts_loc_time_info_t | loc_time_info

## Detailed Description

Current Time Service event.

## Field Documentation

## ◆ conn_idx

uint8_t cts_evt_t::conn_idx

The index of the connection.

## ◆ cur_time

cts_cur_time_t cts_evt_t::cur_time

Curren time set by peer.

## ◆ evt_type

cts_evt_type_t cts_evt_t::evt_type

The CTS event type.

## ◆ length

uint16_t cts_evt_t::length

Length of event data.

## ◆ loc_time_info

cts_loc_time_info_t cts_evt_t::loc_time_info

Local time information set by peer.

## ◆ p_data

const uint8_t* cts_evt_t::p_data

Pointer to event data.

The documentation for this struct was generated from the following file:

- cts.h