Macros
XQSPI Read Command in XIP mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | XQSPI_READ_CMD_READ LL_XQSPI_XIP_CMD_READ
#define | XQSPI_READ_CMD_FAST_READ LL_XQSPI_XIP_CMD_FAST_READ
#define | XQSPI_READ_CMD_DUAL_OUT_READ LL_XQSPI_XIP_CMD_DUAL_OUT_READ
#define | XQSPI_READ_CMD_DUAL_IO_READ LL_XQSPI_XIP_CMD_DUAL_IO_READ
#define | XQSPI_READ_CMD_QUAD_OUT_READ LL_XQSPI_XIP_CMD_QUAD_OUT_READ
#define | XQSPI_READ_CMD_QUAD_IO_READ LL_XQSPI_XIP_CMD_QUAD_IO_READ

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_READ_CMD_DUAL_IO_READ

#define XQSPI_READ_CMD_DUAL_IO_READ LL_XQSPI_XIP_CMD_DUAL_IO_READ

Dual-IO Fast Read mode

## ◆ XQSPI_READ_CMD_DUAL_OUT_READ

#define XQSPI_READ_CMD_DUAL_OUT_READ LL_XQSPI_XIP_CMD_DUAL_OUT_READ

Dual-Out Fast Read mode

## ◆ XQSPI_READ_CMD_FAST_READ

#define XQSPI_READ_CMD_FAST_READ LL_XQSPI_XIP_CMD_FAST_READ

Fast Read mode

## ◆ XQSPI_READ_CMD_QUAD_IO_READ

#define XQSPI_READ_CMD_QUAD_IO_READ LL_XQSPI_XIP_CMD_QUAD_IO_READ

Quad-IO Fast Read mode

## ◆ XQSPI_READ_CMD_QUAD_OUT_READ

#define XQSPI_READ_CMD_QUAD_OUT_READ LL_XQSPI_XIP_CMD_QUAD_OUT_READ

Quad-Out Fast Read mode

## ◆ XQSPI_READ_CMD_READ

#define XQSPI_READ_CMD_READ LL_XQSPI_XIP_CMD_READ

Read mode