Data Fields
ags_init_t Struct Reference
BLE Services » Alexa Gadget Service (AGS) » Structures

Alexa Gadget Service init stucture. This contains all option and data needed for initialization of the service. More...

`#include <ags.h>`

## Data Fields
ags_evt_handler_t | evt_handler
ags_stream_cb_t | ags_control_stream_cb
ags_stream_cb_t | ags_alexa_stream_cb
uint16_t | char_mask

## Detailed Description

Alexa Gadget Service init stucture. This contains all option and data needed for initialization of the service.

## Field Documentation

## ◆ ags_alexa_stream_cb

ags_stream_cb_t ags_init_t::ags_alexa_stream_cb

Callback for incoming Alexa streams.

## ◆ ags_control_stream_cb

ags_stream_cb_t ags_init_t::ags_control_stream_cb

Callback for incoming control streams.

## ◆ char_mask

uint16_t ags_init_t::char_mask

Initial mask of supported characteristics, and configured with Characteristics Mask.

## ◆ evt_handler

ags_evt_handler_t ags_init_t::evt_handler

Alexa Gadget Service event handler.

The documentation for this struct was generated from the following file:

- ags.h