Data Fields
gap_set_pref_slave_evt_dur_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Set preference slave event duration. More...

`#include <ble_gapc.h>`

## Data Fields
uint16_t | duration
uint8_t | single_tx

## Detailed Description

Set preference slave event duration.

## Field Documentation

## ◆ duration

uint16_t gap_set_pref_slave_evt_dur_param_t::duration

Preferred event duration.

## ◆ single_tx

uint8_t gap_set_pref_slave_evt_dur_param_t::single_tx

Slave transmits a single packet per connection event (False/True).

The documentation for this struct was generated from the following file:

- ble_gapc.h