Macros
SCLK Gate
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_SCLKG_NONE (0x00000000UL)
#define | LL_I2S_SCLKG_CYCLES_12 (0x1UL << I2S_CLKCONFIG_SCLKG_Pos)
#define | LL_I2S_SCLKG_CYCLES_16 (0x2UL << I2S_CLKCONFIG_SCLKG_Pos)
#define | LL_I2S_SCLKG_CYCLES_20 (0x3UL << I2S_CLKCONFIG_SCLKG_Pos)
#define | LL_I2S_SCLKG_CYCLES_24 (0x4UL << I2S_CLKCONFIG_SCLKG_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_SCLKG_CYCLES_12

#define LL_I2S_SCLKG_CYCLES_12 (0x1UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 12 sclk cycles.

## ◆ LL_I2S_SCLKG_CYCLES_16

#define LL_I2S_SCLKG_CYCLES_16 (0x2UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 16 sclk cycles.

## ◆ LL_I2S_SCLKG_CYCLES_20

#define LL_I2S_SCLKG_CYCLES_20 (0x3UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 20 sclk cycles.

## ◆ LL_I2S_SCLKG_CYCLES_24

#define LL_I2S_SCLKG_CYCLES_24 (0x4UL << I2S_CLKCONFIG_SCLKG_Pos)

Gating after 24 sclk cycles.

## ◆ LL_I2S_SCLKG_NONE

#define LL_I2S_SCLKG_NONE (0x00000000UL)

Clock gating is disabled.