Macros
Feature Bits
BLE Services » Running Speed and Cadence Service (RSCS) » Defines

Running Speed and Cadence Service feature bits. More...

## Macros
#define | RSCS_FEAT_INSTANT_STRIDE_LEN_BIT (0x01 << 0)
#define | RSCS_FEAT_TOTAL_DISTANCE_BIT (0x01 << 1)
#define | RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT (0x01 << 2)
#define | RSCS_FEAT_CALIBRATION_PROCEDURE_BIT (0x01 << 3)
#define | RSCS_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 4)
#define | RSCS_FEAR_FULL_BIT (0x1f)

## Detailed Description

Running Speed and Cadence Service feature bits.

## Macro Definition Documentation

## ◆ RSCS_FEAR_FULL_BIT

#define RSCS_FEAR_FULL_BIT (0x1f)

Bit for all RSC features Supported.

## ◆ RSCS_FEAT_CALIBRATION_PROCEDURE_BIT

#define RSCS_FEAT_CALIBRATION_PROCEDURE_BIT (0x01 << 3)

Bit for Calibration Procedure Supported.

## ◆ RSCS_FEAT_INSTANT_STRIDE_LEN_BIT

#define RSCS_FEAT_INSTANT_STRIDE_LEN_BIT (0x01 << 0)

Bit for Instantaneous Stride Length Measurement Supported.

## ◆ RSCS_FEAT_MULTIPLE_SENSORS_BIT

#define RSCS_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 4)

Bit for Multiple Sensor Locations Supported.

## ◆ RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT

#define RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT (0x01 << 2)

Bit for Running or Walking Status Supported.

## ◆ RSCS_FEAT_TOTAL_DISTANCE_BIT

#define RSCS_FEAT_TOTAL_DISTANCE_BIT (0x01 << 1)

Bit for Total Distance Measurement Supported.